11/20/2014
=============
This driver is for the XR21x141x USB UART product family.  This driver has been WHQL/HCK-certified on Windows 8.1.  The driver has been tested on
Windows XP/Vista/7/8/8.1. The version is 2.1.0.0.

This zip file contains the following folders:

	x64	= contains the 64-bit driver for 64-bit systems.
	x86	= contains the 32-bit driver for 32-bit systems.	
	EXE	= contains the executable that will uninstall previous driver installations, install the new driver, and search for any USB devices attached to the system.

Revision History (Rev. 2.0 to 2.1):
 - WHQL/HCK certified driver for Windows 8.1.  Driver will also work on Windows XP, Vista, 7 including Win XP Embedded, Win 7 Embedded and Windows Server.
 - Minor fixes to the logic to pass Windows 8.1 HCK testing.

Revision History (Rev. 1.9 to 2.0):
 - WHQL/HCK certified driver for Windows 8.  Driver will also work on Windows XP, Vista, 7 including Win XP Embedded, Win 7 Embedded and Windows Server.
 - Minor fixes to the logic to pass Windows 8 HCK testing.	

Revision History (Rev. 1.8 to 1.9):
 - Logic to override Writing to gpio-mode/dir/intmask, and char-format registers if the otp bit for the same is set in xr21b1411 device is implemented.
 - Failure to transfer using xmodem protocol is fixed.
 - Support for 9-bit mode for xr21v141x devices is enabled.
 - An ioctl is provided to get the VID, PID, and the channel number of the port opened.
 - Wide mode for xr21v141x device was being erroneously set while resuming from standby/hibernation is fixed.
 - Custom driver bit for xr21b1411 is now also set while resuming from standby/hibernation.
 - Gpio direction and int-mask registers are also restored while resuming from standby/hibernation.
 - Issues that were caused while asynchronous writes happen without waiting for the previous write to complete from the app is fixed.


Revision History (Rev. 1.7 to 1.8):
 - Fixed a blue-screen/crash issue when communication errors were generated .
 - Support for LowLatency/WideMode via device manager property pages is added.
 - LowLatency mode is enabled by default for baud-rates <= 50 Kbps.
 - Updated Set/Clr RTS/DTR logic in init and createfile dispatch so that it is on par with the standard uart driver.
 - WideMode support via ioctls calls is added for XR21B1411.
 - Break is turned off when the port is closed by the application, to be in sync with standard driver.
 - Improper state of TxHolding is fixed by updating interrupt endpoint logic. 


Revision History (Rev. 1.6 to 1.7):
 - IOCTL Support for enabling/disabling wide mode is added.
 - Support for turning on/off break is added.
 - LSR status is generated and is processed for any errors.
 - Endpoints are reset if there are any endpoint errors like stalled or halted.
 - Write Timeout logic is fixed and transmit empty event (SERIAL_EV_TXEMPTY) is implemented.
 - Cancelling and freeing of urbs are done in remove-device rather in closing of the ports to fix certain issues.

Revision History (Rev. 1.5 to 1.6):
 - Creating Symbolic link has been updated. This makes sure the Com is opened without any failure 
   even after the device is unplugged and plugged back.
 - Surprise removal portion is updated to avoid some potential issues when the port is closed 
   after the device is unplugged.

Revision History (Rev. 1.4 to 1.5):
 - Support for custom VID/PID - If OEMs want to use xrusbser.sys as is, they need to make sure
   XR21v1410/1412/1414 has even DID and XR21B1411 has odd DID. Otherwise different registers
   are programmed and the operation can not be guaranteed.
 - Fixed the bug that would have crashed the system if the driver is loaded for a phantom device 
   that was not uninstalled/installed properly.
 - IOCTL_SERIAL_GET_MODEMSTATUS now returns the live status of GPIO (reverted back to 1.2 logic). 

Revision History (Rev. 1.3 to 1.4):
 - Support for XR21B1411.
 - WriteTimeout is implemented.

Revision History (Rev. 1.2 to 1.3):
 - Improved data throughput to approximately 9Mbps
 - Fixed default state of RTS# and DTR# pins
 - Fix the usb 2.0 hub issue	
 - Changes in calculating serialstate in interrupt endpoint.