; Windows USB CDC Driver Setup File for Gemscope
; Copyright (c) 2008 Gemalto

[Version] 
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PROVIDER%
LayoutFile=layout.inf
DriverVer=08/04/2008,1.0.0.2
CatalogFile=GCR5500-D.cat

[Manufacturer] 
%MFGNAME%=VirComDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksFiles]
;Not Used only for chkinf test.

[SourceDisksNames]
1=%INSTDISK%,,

[VirComDevice]
%USB\VID_08E6&PID_4000% = DriverInstall, USB\VID_08E6&PID_4000

[VirComDevice.NT]
%USB\VID_08E6&PID_4000% = DriverInstall, USB\VID_08E6&PID_4000

[VirComDevice.NTamd64]
%USB\VID_08E6&PID_4000% = DriverInstall, USB\VID_08E6&PID_4000

[DriverInstall]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.AddReg

[DriverInstall.NT]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NT.AddReg

[DriverInstall.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys 

[Strings] 
PROVIDER    = "Gemalto"
MFGNAME     = "Gemalto GCR5500-D"
USB\VID_08E6&PID_4000="GCR5500-D Virtual Comm port"
SERVICE     = "USB RS-232 Emulation Driver"
INSTDISK="Installation Disc for Virtual Comm port"
