; aec6290.INF  
;        This inf file is for AEC6290 PCI Serial ATA Controller
;        in Windows NT,2000
;
[version]
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}	;SCSI CLASS
Provider=%ProviderName%
LayoutFile=layout.inf

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[ControlFlags]
;
; Exclude the following devices from Select Device list.
; These represent 'combination' driver nodes, for which there are separate items to be
; presented to the user.  These combination nodes are only used when figuring out what
; driver node to associate with a pre-existing service.
;
ExcludeFromSelect = SPARROW_SCSI, ARROW_SCSI, BUSLOGIC_SCSI, DPTSCSI_SCSI, FD16_700_SCSI, ATAPI_SCSI
ExcludeFromSelect = DAC960NT_SCSI, SYMC810_SCSI, NCR53C9X_SCSI, NCRC710_SCSI, FD8XX_SCSI, MITSUMI_SCSI

;
; Exclude the following devices from the platforms where they are not available.
;
ExcludeFromSelect.NTPPC = CPQARRAY_SCSI, DELLDSA_SCSI, *ADP1740, *ADP7770, *ADP7771, *ADP2840, AMI0NT_SCSI, mca_7f4c, mca_7f4d, mca_7f4f, MF\EISA_ZDS2000_DEV2, OLISCSI_SCSI, mca_004e, mca_01ba, *pnpa003, *ctl2001, *pnpA02B, *USC0140, *USC0141
ExcludeFromSelect.NTPPC = mca_01bb, *CPQ4410, *CPQ4411, mca_8eff, *PNPA022, *WDC2001, *FDC0950, *pnpa030, *pnpa031, *pnpa032, *USC0142, *USC0143, *USC0240, FLASHPNT_SCSI, CPQFWS2E_SCSI
ExcludeFromSelect.NTAlpha = mca_7f4c, mca_7f4d, mca_7f4f, MF\EISA_ZDS2000_DEV2, OLISCSI_SCSI, mca_004e, mca_01ba, mca_01bb, *CPQ4410, *CPQ4411, mca_8eff, *PNPA022, *WDC2001, *FDC0950, *pnpa030, *pnpa031, *pnpa032, *pnpa003, *ctl2001, *pnpA02B
ExcludeFromSelect.NTAlpha = *USC0140, *USC0141, *USC0142, *USC0143, *USC0240, FLASHPNT_SCSI, CPQFWS2E_SCSI
ExcludeFromSelect.NTMIPS = MF\EISA_ZDS2000_DEV2, *CPQ4410, *CPQ4411, mca_8eff, *PNPA022, *WDC2001, *FDC0950, *pnpa030, *pnpa031, *pnpa032, *pnpa003, *ctl2001, *pnpA02B, *USC0140, *USC0141, *USC0142, *USC0143, *USC0240, FLASHPNT_SCSI, CPQFWS2E_SCSI

;
; Exclude the generic (non-PCI) IDE description from all platforms.  We can't do this globally (i.e.,
; "ExcludeFromSelect" with no suffix) because then we'll think it was hidden because we wanted that to
; be the migration name.
;
ExcludeFromSelect.NTPPC = *PNP0600
ExcludeFromSelect.NTAlpha = *PNP0600
ExcludeFromSelect.NTMIPS = *PNP0600
ExcludeFromSelect.NTx86 = *PNP0600

[Manufacturer]
%MfgName%=ACARD


;****************************************************
; Manufacturer device list
[ACARD]
%aec6290.DeviceDesc% = aec6290_Inst, PCI\VEN_1191&DEV_0009;&SUBSYS_00091191

[SourceDisksFiles]

[aec6290_Inst]
CopyFiles = @aec6290.sys
Reboot

[aec6290_Inst.Services]
AddService = aec6290, %SPSVCINST_ASSOCSERVICE%, aec6290_Service_Inst, Miniport_EventLog_Inst

[aec6290_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\aec6290.sys                                       ;\SC247XU.sys
LoadOrderGroup = SCSI Miniport

AddReg         = pnpsafe_pci_addreg

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001 ; PCI Bus

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[Strings]
ProviderName = "ACARD"
MfgName = "ACARD"
aec6290.DeviceDesc = "ACARD AEC6290 Serial ATA Controller"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001