; nas241w.inf
; Setup information file for NEC AS241W Monitor
;
; Copyright (C) 2011, NEC Display Solutions,Ltd
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nas241w.cat
DriverVer=09/12/2011,1.11.0912.1510

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC6885

[DestinationDirs]
AS241W.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nas241w.icm=1

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%AS241W%=AS241W.Install, Monitor\NEC6885

[NECDS.ntamd64]
%AS241W%=AS241W.Install.ntamd64, Monitor\NEC6885

[AS241W.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS241W.AddReg, 1920, DPMS
CopyFiles=AS241W.CopyFiles

[AS241W.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS241W.AddReg, 1920, DPMS
CopyFiles=AS241W.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1920]
HKR,,MaxResolution,,"1920,1080"

[DPMS]
HKR,,DPMS,,1

[AS241W.AddReg]
;HKR,"MODES\1920,1080",Mode1,,"31.0-83.0,55.0-76.0,+,+"
HKR,,ICMProfile,0,"nas241w.icm"

[AS241W.CopyFiles]
nas241w.icm

[Strings]
NECDS="NEC"
AS241W="NEC AS241W"
Disk1="NEC Monitor Installation Disk"
