;
; Installation inf file for MOD7700 driver
; Copyright 2005, DiBcom SA

[Version]
signature	= "$CHICAGO$"
Class		= Media
ClassGUID	= {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider	= %Dibcom%
DriverVer	= 07/09/2007,3.9.0.0
CatalogFile 	= mod7700.cat


[Manufacturer]
%MfgName% = DIBCOM,NTamd64


[DIBCOM]
%MOD7000.DeviceDesc% 	= MOD7000.Device,USB\VID_1044&PID_7002				; STK7700PH (7700C)

[DIBCOM.NTamd64]
%MOD7000.DeviceDesc% 	= MOD7000.Device,USB\VID_1044&PID_7002				; STK7700PH (7700C)

[DestinationDirs]
MOD7000.CopyDrivers	= 12,


[SourceDisksNames]
1 = %INSTALLATION_DISK%,,


[SourceDisksFiles]
mod7700.sys = 1


[ControlFlags]
ExcludeFromSelect    = *
ExcludeFromSelect.NT = *


[MOD7000.Device]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = MOD7000.CopyDrivers


[MOD7000.Device.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = MOD7000.CopyDrivers

[MOD7000.Device.NT.HW]
AddReg = MOD7000_DEVICE_AddReg


[MOD7000.Device.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService


[MOD7000.AddService]
DisplayName    = %MOD7000.FriendlyName%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\mod7700.sys
LoadOrderGroup = Base
AddReg         = MOD7000.Service.AddReg


[MOD7000.Service.AddReg]
HKR,,DigitalJmp,0x00010001,0x00
HKR,"parameters","ReducedScanning",0x0000001,0x00

[MOD7000.CopyDrivers]
mod7700.sys


[MOD7000.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,mod7700.sys
HKR,,PageOutWhenUnopened,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audio input"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"

[MOD7000_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001EFC
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"DiBcom BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"DiBcom BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"DiBcom BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"DiBcom BDA Analog Capture"
HKR,,"AnlgCaptureDefaultStandard",0x00010001,0x00000000
HKR,,"AnlgXBarFilterName",0,"DiBcom BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"DiBcom BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"DiBcom Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"DiBcom BDA Analog Audio Capture"

[Strings]

;Pin Id
HOOK_ANLG_AUDIO_IN_PIN  = "{356A9E15-B6B8-4066-A381-B531C606A200}"
HOOK_ANLG_AUDIO_OUT_PIN = "{0A95FEC0-4617-4f93-9861-91C9E59E1C09}"


Dibcom               	= "Dibcom"
MfgName              	= "DIBCOM"
MOD7000.DeviceDesc   	= "Gigabyte U8000 TV tuner device"
MOD7070.DeviceDesc   	= "DiBcom DIB7070 based TV tuner device"
MOD7000.FriendlyName 	= "DiBcom based TV tuner device"
INSTALLATION_DISK    	= "DiBcom Installation Disk"

;
; The following items should be moved to KS_registration - TCP
;

MediaCategories         = "SYSTEM\CurrentControlSet\Control\MediaCategories"
    

;
; ServiceType values
SERVICE_KERNEL_DRIVER			= 0x00000001
SERVICE_FILE_SYSTEM_DRIVER		= 0x00000002
SERVICE_ADAPTER					= 0x00000004
SERVICE_RECOGNIZER_DRIVER		= 0x00000008
SERVICE_WIN32_OWN_PROCESS		= 0x00000010
SERVICE_WIN32_SHARE_PROCESS		= 0x00000020
SERVICE_INTERACTIVE_PROCESS		= 0x00000100
SERVICE_INTERACTIVE_SHARE_PROCESS	= 0x00000120

; StartType values
SERVICE_BOOT_START          = 0x00000000
SERVICE_SYSTEM_START        = 0x00000001
SERVICE_AUTO_START          = 0x00000002
SERVICE_DEMAND_START        = 0x00000003
SERVICE_DISABLED            = 0x00000004

; ErrorControl values
SERVICE_ERROR_IGNORE        = 0x00000000
SERVICE_ERROR_NORMAL        = 0x00000001
SERVICE_ERROR_SEVERE        = 0x00000002
SERVICE_ERROR_CRITICAL      = 0x00000003

; Characteristic flags
NCF_VIRTUAL                 = 0x0001
NCF_WRAPPER                 = 0x0002
NCF_PHYSICAL                = 0x0004
NCF_HIDDEN                  = 0x0008
NCF_NO_SERVICE              = 0x0010
NCF_NOT_USER_REMOVABLE      = 0x0020
NCF_HAS_UI                  = 0x0080
NCF_MODEM                   = 0x0100

; Registry types
REG_MULTI_SZ                = 0x10000
REG_EXPAND_SZ               = 0x20000
REG_DWORD                   = 0x10001

; Win9x Compatible Types
REG_BINARY                  = 17
REG_SZ                      = 0

; Service install flags
SPSVCINST_TAGTOFRONT        = 0x1
SPSVCINST_ASSOCSERVICE      = 0x2
