;
; Installation inf file for DVB-S USB adapter BDA driver
; Copyright 2009-2010, DTV-DVB

[Version]
signature	= "$CHICAGO$"
Class		= Media
ClassGUID	= {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider	= %DTV-DVB%
DriverVer	= 08/20/2010,1.0.8.100
CatalogFile         = AzureWaveUsbBda.cat
CatalogFile.NTAMD64 = AMD64\AzureWaveUsbBda.cat
CatalogFile.NTIA64  = IA64\AzureWaveUsbBda.cat

[Manufacturer]
%MfgName% = DTV-DVB, NTAMD64, NTIA64

[DTV-DVB]
;azurewave ids
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3344
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3344
;6033(-s/s2)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3285
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3285

;terratec s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10AC
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10AC

;6027
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A9
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A9
;6017
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A6
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A6
;elgato s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0025
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0025
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_002A
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_002A
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0036
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0036
;elgato 6007
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0026
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0026

;terratec h7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_008F
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_008F

;technisat skystar
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0001
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0001

;technisat 6027
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0002
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0002

;technisat -t/-c combo
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0003
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0003

;6011(T/C Siliconlab)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3290
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3290

;6035 wireless DVB-S
%AzureWaveUsbBda.WirelessDesc%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3292

;6038(-S/-S2)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3343
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3343

[DTV-DVB.NTAMD64]
;azurewave ids
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3285
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3285

;terratec s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10AC
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10AC

;elgato s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0025
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0025
;6027-E
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3344
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3344

;elgato 6007
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0026
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0026
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_002A
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_002A

;6017
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A9
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A9
;terratec h7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_008F
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_008F

;6017
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A6
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A6

;technisat skystar
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0001
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0001

;technisat 6027
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0002
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0002

;technisat -t/-c combo
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0003
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0003

;6011(t/c siliconlab)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3290
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3290

;6035 wireless DVB-S
%AzureWaveUsbBda.WirelessDesc%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3292

[DTV-DVB.NTIA64]
;azurewave ids
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3245
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3246
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3209
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3268
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3229
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3347
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3275
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3285
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3285

;terratec s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A4
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10AC
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10AC

;elgato s7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0025
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0025
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_002A
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_002A
;6027-E
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3344
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3344

;elgato 6007
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0FD9&PID_0026
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0FD9&PID_0026

;6017
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A9
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A9
;terratec h7
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_10A3
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_008F
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_008F

;6017
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_0CCD&PID_00A6
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_0CCD&PID_00A6

;technisat skystar
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0001
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0001

;technisat 6027
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0002
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0002

;technisat -t/-c combo
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_14F7&PID_0003
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_14F7&PID_0003

;6011(T/C Siliconlab)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3290
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3290

;6035 wireless DVB-S
%AzureWaveUsbBda.WirelessDesc%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3292

;6038(-S/-S2)
%AzureWaveUsbBda.DeviceDesc%	= AzureWaveUsbBda.Device,USB\VID_13D3&PID_3343
%AzureWaveUsbBda.DeviceDesc1%	= AzureWaveUsbBda.Device1,USB\VID_13D3&PID_3343

[DestinationDirs]
AzureWaveUsbBda.CopyDrivers	= 10,System32\Drivers 


[SourceDisksNames]
1 = %INSTALLATION_DISK%, AzureWaveUsbBda.inf, ,

[SourceDisksNames.AMD64]
1 = %INSTALLATION_DISK%, AzureWaveUsbBda.inf, , \AMD64

[SourceDisksNames.IA64]
1 = %INSTALLATION_DISK%, AzureWaveUsbBda.inf, , \IA64

[SourceDisksFiles]
AzureWaveUsbBda.sys = 1


[ControlFlags]
ExcludeFromSelect	= *
ExcludeFromSelect.NT	= *


[AzureWaveUsbBda.Device.NT]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = AzureWaveUsbBda.AddReg
CopyFiles  = AzureWaveUsbBda.CopyDrivers


[AzureWaveUsbBda.Device.NT.Services]
Addservice = AzureWaveUsbBda, 0x00000002, AzureWaveUsbBda.AddService

[AzureWaveUsbBda.Device1.NT]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = AzureWaveUsbBda.AddReg1
CopyFiles  = AzureWaveUsbBda.CopyDrivers


[AzureWaveUsbBda.Device1.NT.Services]
Addservice = AzureWaveUsbBda, 0x00000002, AzureWaveUsbBda.AddService

[AzureWaveUsbBda.AddService]
DisplayName    = %AzureWaveUsbBda.FriendlyName%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\AzureWaveUsbBda.sys
LoadOrderGroup = Base

[AzureWaveUsbBda.CopyDrivers]
AzureWaveUsbBda.sys


[AzureWaveUsbBda.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,AzureWaveUsbBda.sys
HKR,,PageOutWhenUnopened,3,01

;Disabe HID driver install
HKR,"ENUM\Device1",pnpid,,"AzureWaveusbHid.VIRTUAL"

HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088}
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39}
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67}
HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E}
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080}
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75}
HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30}
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4}
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4},Name,,"Antenna In Pin"

; LNBLOFLowBand = 9750  MHz
HKR,"DriverData","LNBLOFLowBand",0x00010001, 0x16,0x26,0x00,0x00
; LNBLOFHighBand = 10600 MHz
HKR,"DriverData","LNBLOFHighBand",0x00010001, 0x68,0x29,0x00,0x00
; LNBLOF Low/High band switch, 11700 MHz
HKR,"DriverData","LNBLOFHiLoSwitch",0x00010001, 0xb4,0x2d,0x00,0x00


; DiSEqC Selection
; 0: Normal
HKR,"DriverData","DiSEqC",0x00010001, 0x00,0x00,0x00,0x00
; 1: DiSEqC A
;HKR,"DriverData","DiSEqC",0x00010001, 0x01,0x00,0x00,0x00
; 2: DiSEqC B
;HKR,"DriverData","DiSEqC",0x00010001, 0x02,0x00,0x00,0x00
; 3: DiSEqC C
;HKR,"DriverData","DiSEqC",0x00010001, 0x03,0x00,0x00,0x00
; 4: DiSEqC D
;HKR,"DriverData","DiSEqC",0x00010001, 0x04,0x00,0x00,0x00

; LNB Power
; 0: OFF
;HKR,"DriverData","LNBPower",0x00010001, 0x00,0x00,0x00,0x00
; 1: ON
HKR,"DriverData","LNBPower",0x00010001, 0x01,0x00,0x00,0x00

; 22k Tone
; 0: ON/OFF by LNB switch frequency
;HKR,"DriverData","Tone",0x00010001, 0x00,0x00,0x00,0x00
; 1: OFF
HKR,"DriverData","Tone",0x00010001, 0x01,0x00,0x00,0x00
; 2: ON
;HKR,"DriverData","Tone",0x00010001, 0x02,0x00,0x00,0x00

; Tone and Data Burst
; 0: Tone and data burst off
HKR,"DriverData","ToneDataBurst",0x00010001, 0x00,0x00,0x00,0x00
; 1: Tone burst on
;HKR,"DriverData","ToneDataBurst",0x00010001, 0x01,0x00,0x00,0x00
; 2: Data burst on
;HKR,"DriverData","ToneDataBurst",0x00010001, 0x02,0x00,0x00,0x00

; IR system code checklist1
; 00 00 00 00 : Enable all
; FF FF 00 00 : Filter All
HKR,"DriverData","IRSYSCODECHECK1",0x00010001, 0xFF,0x00,0x00,0x00

; //Mapping RC table for DTV-DVB
HKR,"DriverData","RC_Configuration",0x00010001, 0x00,0x00,0x00,0x00
; //Mapping RC table for Cyberlink
;HKR,"DriverData","RC_Configuration",0x00010001, 0x01,0x00,0x00,0x00
; //Mapping RC table for IVI
;HKR,"DriverData","RC_Configuration",0x00010001, 0x02,0x00,0x00,0x00
; //Mapping RC table for MCE
;HKR,"DriverData","RC_Configuration",0x00010001, 0x03,0x00,0x00,0x00
; //Mapping RC table for NEW TH HID RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0x04,0x00,0x00,0x00
; //Mapping RC table for Custom
;HKR,"DriverData","RC_Configuration",0x00010001, 0x05,0x00,0x00,0x00
; //Mapping RC table for DNTVLive HID RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0x10,0x00,0x00,0x00
; //Disable RC
;HKR,"DriverData","RC_Configuration",0x00010001, 0xFF,0xFF,0x00,0x00

; TSGenSimulator
; 0:Disabled, 1:DVB-S, 2:DVB-T, 4:DVB-C, 8:ATSC 16:MCE DVB-T
HKR,"DriverData","TSGenSimulator",0x00010001, 0x00,0x00,0x00,0x00

; SupportHWInfo (MAX 32 bytes)
HKR,"DriverData","SupportHWInfo",0x00010000, "7050 DVB-S TVBox"

; Device_Name (MAX 32 bytes)
;HKR,"DriverData","Device_Name",0x00010000, "7050 USB-Sat"

;Temp Key For Save Ts File
HKR,"DriverData","BuildTsFile",0x00010001, 0x00,0x00,0x00,0x00

;UploadMicrocode for 6007
HKR,"DriverData","UploadMicrocode",0x00010001, 0x01,0x00,0x00,0x00

;Antenna Switch, enable default
HKR,"DriverData","EnableSwitchAntenna",0x00010001, 0x01,0x00,0x00,0x00

;Antenna Auto Switch, disable default, ignored if EnableSwitchAntenna not set
HKR,"DriverData","AutoSwitchAntenna",0x00010001, 0x00,0x00,0x00,0x00

;Time delay for antenna switch ready, 20ms default
HKR,"DriverData","AntennaSwitchDelay",0x00010001, 0x14,0x00,0x00,0x00

;scan both DVB-S/S2 mode
HKR,"DriverData","EnableDualSModeScan",0x00010001, 0x01,0x00,0x00,0x00

;powersaving time:5Min
HKR,"DriverData","PowerSaveTimeOut",0x00010001, 0x96,0x00,0x00,0x00

; tuner names(MAX 128 bytes)
HKR,"DriverData","DVBSTunerName",0x00010000, "DTV-DVB BDA DVBS Tuner"
HKR,"DriverData","DVBTTunerName",0x00010000, "DTV-DVB BDA DVBT Tuner"
HKR,"DriverData","DVBCTunerName",0x00010000, "DTV-DVB BDA DVBC Tuner"
HKR,"DriverData","DVBSCaptureName",0x00010000, "DTV-DVB BDA DVBS Capture"
HKR,"DriverData","DVBTCaptureName",0x00010000, "DTV-DVB BDA DVBT Capture"
HKR,"DriverData","DVBCCaptureName",0x00010000, "DTV-DVB BDA DVBC Capture"

[AzureWaveUsbBda.AddReg1]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,AzureWaveUsbBda.sys
HKR,,PageOutWhenUnopened,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{2700E515-7868-4e6f-A57E-0D55A850EC7D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088}
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{142DC0CE-6F84-451f-B359-EF15BBA30088},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39}
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{CA00E3F6-190E-40c0-BD9E-69CB46145A39},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67}
HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{C7037B65-78D8-4966-BDA0-704A43B37A67},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E}
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{0FDBFE87-05CA-4778-ABE5-EE5E75E7EA5E},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080}
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{D7C789A8-11B9-45a8-AF1C-67791C440080},Name,,"Antenna In Pin"

HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75}
HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{1F06247C-D6C9-45b4-9CAA-79345818EB75},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30}
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{5943F8C7-46E6-4070-9900-B265D14FEF30},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4}
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{B2F9FD35-121E-4d5b-8EDF-CDB4472F0DD4},Name,,"Antenna In Pin"


; LNBLOFLowBand = 9750  MHz
HKR,"DriverData","LNBLOFLowBand",0x00010001, 0x16,0x26,0x00,0x00
; LNBLOFHighBand = 10600 MHz
HKR,"DriverData","LNBLOFHighBand",0x00010001, 0x68,0x29,0x00,0x00
; LNBLOF Low/High band switch, 11700 MHz
HKR,"DriverData","LNBLOFHiLoSwitch",0x00010001, 0xb4,0x2d,0x00,0x00


; DiSEqC Selection
; 0: Normal
HKR,"DriverData","DiSEqC",0x00010001, 0x00,0x00,0x00,0x00
; 1: DiSEqC A
;HKR,"DriverData","DiSEqC",0x00010001, 0x01,0x00,0x00,0x00
; 2: DiSEqC B
;HKR,"DriverData","DiSEqC",0x00010001, 0x02,0x00,0x00,0x00
; 3: DiSEqC C
;HKR,"DriverData","DiSEqC",0x00010001, 0x03,0x00,0x00,0x00
; 4: DiSEqC D
;HKR,"DriverData","DiSEqC",0x00010001, 0x04,0x00,0x00,0x00

; LNB Power
; 0: OFF
;HKR,"DriverData","LNBPower",0x00010001, 0x00,0x00,0x00,0x00
; 1: ON
HKR,"DriverData","LNBPower",0x00010001, 0x01,0x00,0x00,0x00

; 22k Tone
; 0: ON/OFF by LNB switch frequency
HKR,"DriverData","Tone",0x00010001, 0x00,0x00,0x00,0x00
; 1: OFF
;HKR,"DriverData","Tone",0x00010001, 0x01,0x00,0x00,0x00
; 2: ON
;HKR,"DriverData","Tone",0x00010001, 0x02,0x00,0x00,0x00

; Tone and Data Burst
; 0: Tone and data burst off
HKR,"DriverData","ToneDataBurst",0x00010001, 0x00,0x00,0x00,0x00
; 1: Tone burst on
;HKR,"DriverData","ToneDataBurst",0x00010001, 0x01,0x00,0x00,0x00
; 2: Data burst on
;HKR,"DriverData","ToneDataBurst",0x00010001, 0x02,0x00,0x00,0x00

; TSGenSimulator
; 0:Disabled, 1:DVB-S, 2:DVB-T, 4:DVB-C, 8:ATSC 16: MCE DVB-T
HKR,"DriverData","TSGenSimulator",0x00010001, 0x00,0x00,0x00,0x00

; SupportHWInfo (MAX 32 bytes)
HKR,"DriverData","SupportHWInfo",0x00010000, "7050 DVB-S TVBox"

; Device_Name (MAX 32 bytes)
;HKR,"DriverData","Device_Name",0x00010000, "7050 USB-Sat"

;Temp Key For Save Ts File
HKR,"DriverData","BuildTsFile",0x00010001, 0x00,0x00,0x00,0x00

;UploadMicrocode for 6007
HKR,"DriverData","UploadMicrocode",0x00010001, 0x01,0x00,0x00,0x00

;Antenna Switch, enable default
HKR,"DriverData","EnableSwitchAntenna",0x00010001, 0x01,0x00,0x00,0x00

;Antenna Auto Switch, disable default, ignored if EnableSwitchAntenna not set
HKR,"DriverData","AutoSwitchAntenna",0x00010001, 0x00,0x00,0x00,0x00

;Time delay for antenna switch ready, 20ms default
HKR,"DriverData","AntennaSwitchDelay",0x00010001, 0x14,0x00,0x00,0x00

;powersaving time:5Min
HKR,"DriverData","PowerSaveTimeOut",0x00010001, 0x96,0x00,0x00,0x00

; tuner names(MAX 128 bytes)
HKR,"DriverData","DVBSTunerName",0x00010000, "DTV-DVB BDA DVBS Tuner"
HKR,"DriverData","DVBTTunerName",0x00010000, "DTV-DVB BDA DVBT Tuner"
HKR,"DriverData","DVBCTunerName",0x00010000, "DTV-DVB BDA DVBC Tuner"
HKR,"DriverData","DVBSCaptureName",0x00010000, "DTV-DVB BDA DVBS Capture"
HKR,"DriverData","DVBTCaptureName",0x00010000, "DTV-DVB BDA DVBT Capture"
HKR,"DriverData","DVBCCaptureName",0x00010000, "DTV-DVB BDA DVBC Capture"

[Strings]
DTV-DVB				= "DTV-DVB"
MfgName				= "DTV-DVB"
AzureWaveUsbBda.CLSID		= "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"  ; KsProxy.ax's ID, REQUIRED
AzureWaveUsbBda.DeviceDesc		= "DTV-DVB AzureWave DVB USB Box"
AzureWaveUsbBda.DeviceDesc1		= "DTV-DVB AzureWave DVB USB Box(Without HID)"
AzureWaveUsbBda.WirelessDesc		= "Wireless TV Satellite"

INSTALLATION_DISK 		= "DTV-DVB AzureWaveUsbBda Installation Disk"

AzureWaveUsbBda.FriendlyName	= "DTV-DVB AzureWaveUsbBda Tuner"

; ServiceType values
SERVICE_KERNEL_DRIVER				= 0x00000001
SERVICE_FILE_SYSTEM_DRIVER			= 0x00000002
SERVICE_ADAPTER					= 0x00000004
SERVICE_RECOGNIZER_DRIVER			= 0x00000008
SERVICE_WIN32_OWN_PROCESS			= 0x00000010
SERVICE_WIN32_SHARE_PROCESS			= 0x00000020
SERVICE_INTERACTIVE_PROCESS			= 0x00000100
SERVICE_INTERACTIVE_SHARE_PROCESS	        = 0x00000120

; StartType values
SERVICE_BOOT_START          = 0x00000000
SERVICE_SYSTEM_START        = 0x00000001
SERVICE_AUTO_START          = 0x00000002
SERVICE_DEMAND_START        = 0x00000003
SERVICE_DISABLED            = 0x00000004

; ErrorControl values
SERVICE_ERROR_IGNORE        = 0x00000000
SERVICE_ERROR_NORMAL        = 0x00000001
SERVICE_ERROR_SEVERE        = 0x00000002
SERVICE_ERROR_CRITICAL      = 0x00000003

; Characteristic flags
NCF_VIRTUAL                 = 0x0001
NCF_WRAPPER                 = 0x0002
NCF_PHYSICAL                = 0x0004
NCF_HIDDEN                  = 0x0008
NCF_NO_SERVICE              = 0x0010
NCF_NOT_USER_REMOVABLE      = 0x0020
NCF_HAS_UI                  = 0x0080
NCF_MODEM                   = 0x0100

; Registry types
REG_MULTI_SZ                = 0x10000
REG_EXPAND_SZ               = 0x20000
REG_DWORD                   = 0x10001

; Win9x Compatible Types
REG_BINARY                  = 17
REG_SZ                      = 0

; Service install flags
SPSVCINST_TAGTOFRONT        = 0x1
SPSVCINST_ASSOCSERVICE      = 0x2
