;-----------------------------------------------------------------------
;	Driver Inf File
;	
;       Copyright (c) YUAN High Tech Development Co. Ltd. 
;       All Rights Reserved.
;------------------------------------------------------------------------
[Version]
signature                              =         "$CHICAGO$"
Class                                  =         Media
ClassGUID                              =         {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider                               =         %Company%
DriverVer                              =         11/23/2011,6.0.111.19
CatalogFile                            =         cxRDU253Sx86.cat

[Manufacturer]
%Company%                              =         Conexant, NTx86

[SourceDisksNames]
1                                      =         "Conexant Polaris Drivers",,,""

[SourceDisksFiles]
cxRDU253S.sys                          =         1
cxPolarIR.sys                          =         1
cpnotify.ax                            =         1
merlinD.rom                            =         1

[Conexant.NTx86]
;CAPTURE ONLY
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10B0&MI_00            ; AVS ONLY  W/O AUDIO PIN 
%CXPOLARIS.CAPTURE%                    =         POLARIS.CAPTURE,   USB\VID_1164&PID_10B0&MI_01            ;								HID BY USER
%CXPOLARIS.CAPTURE%                    =         POLARIS.CAPTURE,   USB\VID_1164&PID_10B6&MI_01            ; 								HID RC6 (MICROSOFT)
 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10B9&MI_00            ; AVS ONLY  W/O AUDIO PIN		W/O  HID 
%CXPOLARIS.CAPTURE%                    =         POLARIS.CAPTURE,   USB\VID_1164&PID_10B9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10A0&MI_00            ; AVS ONLY
%CXPOLARIS.CAPTURE%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_10A0&MI_01            ;								HID BY USER 
%CXPOLARIS.CAPTURE%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_10A6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10A9&MI_00            ; AVS ONLY						W/O  HID
%CXPOLARIS.CAPTURE%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_10A9&MI_01            ; 

; MXL301
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10C0&MI_00            ; ANALOG ONLY      AVS     FM 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10C0&MI_01            ; 								HID BY USER 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10C6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10D0&MI_00            ; ANALOG ONLY      AVS W/O FM  
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10D0&MI_01            ;								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10D6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10E0&MI_00            ; ANALOG ONLY  W/O AVS     FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10E0&MI_01            ; 								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10E6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_10F0&MI_00            ; ANALOG ONLY  W/O AVS W/O FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10F0&MI_01            ; 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10F6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10C9&MI_00            ; ANALOG ONLY      AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10C9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10D9&MI_00            ; ANALOG ONLY      AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10D9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10E9&MI_00            ; ANALOG ONLY  W/O AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10E9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_10F9&MI_00            ; ANALOG ONLY  W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_10F9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1FC0&MI_00            ; S5H1411          AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FC0&MI_01            ;								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1FD0&MI_00            ; S5H1411          AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FD0&MI_01            ;								HID BY USER 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1FE0&MI_00            ; S5H1411      W/0 AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FE0&MI_01            ;								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1FF0&MI_00            ; S5H1411      W/O AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FF0&MI_01            ;								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1FC9&MI_00            ; S5H1411          AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FC9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1FD9&MI_00            ; S5H1411          AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FD9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1FE9&MI_00            ; S5H1411      W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FE9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1FF9&MI_00            ; S5H1411      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1FF9&MI_01            ;

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1EC0&MI_00            ; RTL2832          AVS     FM  
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EC0&MI_01            ;								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1ED0&MI_00            ; RTL2832          AVS W/O FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1ED0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1ED6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1EE0&MI_00            ; RTL2832      W/O AVS     FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EE0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1EF0&MI_00            ; RTL2832      W/O AVS W/O FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EF0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1EC9&MI_00            ; RTL2832          AVS     FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EC9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1ED9&MI_00            ; RTL2832          AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1ED9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1EE9&MI_00            ; RTL2832      W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1EF9&MI_00            ; RTL2832      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1EF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1DC0&MI_00            ; RTL2836          AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DC0&MI_01            ; 								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1DD0&MI_00            ; RTL2836          AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DD0&MI_01            ; 								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1DE0&MI_00            ; RTL2836      W/O AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DE0&MI_01            ; 								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1DF0&MI_00            ; RTL2836      W/O AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DF0&MI_01            ; 								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DC9&MI_00            ; RTL2836          AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DD9&MI_00            ; RTL2836          AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DE9&MI_00            ; RTL2836      W/O AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DF9&MI_00            ; RTL2836      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1CC0&MI_00            ; DRXJ             AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CC0&MI_01            ; 								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1CD0&MI_00            ; DRXJ             AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CD0&MI_01            ; 								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1CE0&MI_00            ; DRXJ         W/O AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CE0&MI_01            ; 								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1CF0&MI_00            ; DRXJ         W/O AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CF0&MI_01            ; 								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1CC9&MI_00            ; DRXJ             AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1CD9&MI_00            ; DRXJ             AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1CE9&MI_00            ; DRXJ         W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1CF9&MI_00            ; DRXJ         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1CF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1BC0&MI_00            ; DRXK             AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BC0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1BD0&MI_00            ; DRXK             AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BD0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1BE0&MI_00            ; DRXK         W/O AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BE0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1BF0&MI_00            ; DRXK         W/O AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BF0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1BC9&MI_00            ; DRXK             AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1BD9&MI_00            ; DRXK             AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1BE9&MI_00            ; DRXK         W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1BF9&MI_00            ; DRXK         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1BF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1AC0&MI_00            ; DVBT/ATSC        AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AC0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AC6&MI_01            ; 								HID RC6 (MICROSOFT)
 
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1AD0&MI_00            ; DVBT/ATSC        AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AD0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1AE0&MI_00            ; DVBT/ATSC    W/O AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AE0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_1AF0&MI_00            ; DVBT/ATSC    W/O AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AF0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_1AF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1AC9&MI_00            ; DVBT/ATSC        AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_1AC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1AD9&MI_00            ; DVBT/ATSC        AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_1AD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1AE9&MI_00            ; DVBT/ATSC    W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_1AE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1AF9&MI_00            ; DVBT/ATSC    W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_1AF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19C0&MI_00            ; LGDT3305         AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19C0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19C6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19D0&MI_00            ; LGDT3305         AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19D0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19D6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19E0&MI_00            ; LGDT3305     W/O AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19E0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19E6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19F0&MI_00            ; LGDT3305     W/O AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19F0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19F6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_19C9&MI_00            ; LGDT3305         AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19C9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_19D9&MI_00            ; LGDT3305         AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19D9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_19E9&MI_00            ; LGDT3305     W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19E9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_19F9&MI_00            ; LGDT3305     W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19F9&MI_01            ;

; MXL202/MXL301 V09
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_20C0&MI_00            ; ANALOG ONLY      AVS     FM  
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20C0&MI_01            ;  								HID BY USER 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20C6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_20D0&MI_00            ; ANALOG ONLY      AVS W/O FM  
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30D0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30D6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_20E0&MI_00            ; ANALOG ONLY  W/O AVS     FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20E0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20E6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_20F0&MI_00            ; ANALOG ONLY  W/O AVS W/O FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20F0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20F6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_20C9&MI_00            ; ANALOG ONLY      AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20C9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_20D9&MI_00            ; ANALOG ONLY      AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20D9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_20E9&MI_00            ; ANALOG ONLY  W/O AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20E9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_20F9&MI_00            ; ANALOG ONLY  W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_20F9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2FC0&MI_00            ; S5H1411          AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FC0&MI_01            ; 								HID BY USER 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2FD0&MI_00            ; S5H1411          AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FD0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2FE0&MI_00            ; S5H1411      W/0 AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FE0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2FF0&MI_00            ; S5H1411      W/O AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FF0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2FC9&MI_00            ; S5H1411          AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2FD9&MI_00            ; S5H1411          AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2FE9&MI_00            ; S5H1411      W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2FF9&MI_00            ; S5H1411      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2FF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2EC0&MI_00            ; RTL2832          AVS     FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2ED0&MI_00            ; RTL2832          AVS W/O FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2ED0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2ED6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2EE0&MI_00            ; RTL2832      W/O AVS     FM
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2EF0&MI_00            ; RTL2832      W/O AVS W/O FM 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2EC9&MI_00            ; RTL2832          AVS     FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2ED9&MI_00            ; RTL2832          AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2ED9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2EE9&MI_00            ; RTL2832      W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2EF9&MI_00            ; RTL2832      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2EF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2DC0&MI_00            ; RTL2836          AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DC0&MI_01            ;  								HID BY USER 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2DD0&MI_00            ; RTL2836          AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2DE0&MI_00            ; RTL2836      W/O AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2DF0&MI_00            ; RTL2836      W/O AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2DC9&MI_00            ; RTL2836          AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2DD9&MI_00            ; RTL2836          AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2DE9&MI_00            ; RTL2836      W/O AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2DF9&MI_00            ; RTL2836      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2DF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2CC0&MI_00            ; DRXJ             AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CC0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2CD0&MI_00            ; DRXJ             AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CD0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2CE0&MI_00            ; DRXJ         W/O AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CE0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2CF0&MI_00            ; DRXJ         W/O AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CF0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2CC9&MI_00            ; DRXJ             AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2CD9&MI_00            ; DRXJ             AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2CE9&MI_00            ; DRXJ         W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2CF9&MI_00            ; DRXJ         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_2CF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2BC0&MI_00            ; DRXK             AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2BD0&MI_00            ; DRXK             AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2BE0&MI_00            ; DRXK         W/O AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2BF0&MI_00            ; DRXK         W/O AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2BC9&MI_00            ; DRXK             AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2BD9&MI_00            ; DRXK             AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2BE9&MI_00            ; DRXK         W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2BF9&MI_00            ; DRXK         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2BF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2AC0&MI_00            ; DVBT/ATSC        AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2AD0&MI_00            ; DVBT/ATSC        AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2AE0&MI_00            ; DVBT/ATSC    W/O AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_2AF0&MI_00            ; DVBT/ATSC    W/O AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_2AF6&MI_01            ;

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2AC9&MI_00            ; DVBT/ATSC        AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_2AC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2AD9&MI_00            ; DVBT/ATSC        AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_2AD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2AE9&MI_00            ; DVBT/ATSC    W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_2AE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_2AF9&MI_00            ; DVBT/ATSC    W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC%                  =         POLARIS.RDU253S,   USB\VID_1164&PID_2AF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19C0&MI_00            ; LGDT3305         AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19C0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19C6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19D0&MI_00            ; LGDT3305         AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19D0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19D6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19E0&MI_00            ; LGDT3305     W/O AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19E0&MI_01            ; 								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19E6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_19F0&MI_00            ; LGDT3305     W/O AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19F0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_19F6&MI_01            ;								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_29C9&MI_00            ; LGDT3305         AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_29C9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_29D9&MI_00            ; LGDT3305         AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_29D9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_29E9&MI_00            ; LGDT3305     W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_29E9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_29F9&MI_00            ; LGDT3305     W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_29F9&MI_01            ;

;;TDA18272
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_30C0&MI_00            ; ANALOG ONLY      AVS     FM  
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30C0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30C6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_30D0&MI_00            ; ANALOG ONLY      AVS W/O FM  
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30D0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30D6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_30E0&MI_00            ; ANALOG ONLY  W/O AVS     FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30E0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30E6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_30F0&MI_00            ; ANALOG ONLY  W/O AVS W/O FM
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30F0&MI_01            ;  								HID BY USER
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30F6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_30C9&MI_00            ; ANALOG ONLY      AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30C9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_30D9&MI_00            ; ANALOG ONLY      AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30D9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_30E9&MI_00            ; ANALOG ONLY  W/O AVS     FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30E9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_30F9&MI_00            ; ANALOG ONLY  W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ANALOG%                     =         POLARIS.RDU253S,   USB\VID_1164&PID_30F9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3FC0&MI_00            ; S5H1411          AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FC0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3FD0&MI_00            ; S5H1411          AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FD0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3FE0&MI_00            ; S5H1411      W/0 AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FE0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3FF0&MI_00            ; S5H1411      W/O AVS W/0 FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FF0&MI_01            ;   								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3FC9&MI_00            ; S5H1411          AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3FD9&MI_00            ; S5H1411          AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3FE9&MI_00            ; S5H1411      W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3FF9&MI_00            ; S5H1411      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3FF9&MI_01            ; 
  
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3EC0&MI_00            ; RTL2832          AVS     FM
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3ED0&MI_00            ; RTL2832          AVS W/O FM
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3ED0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3ED6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3EE0&MI_00            ; RTL2832      W/O AVS     FM
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EE6&MI_01            ; 								HID RC6 (MICROSOFT)
 
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3EF0&MI_00            ; RTL2832      W/O AVS W/O FM
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EF0&MI_01            ;  								HID BY USER 
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3EC9&MI_00            ; RTL2832          AVS     FM	W/O HID 
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3ED9&MI_00            ; RTL2832          AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3ED9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3EE9&MI_00            ; RTL2832      W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3EF9&MI_00            ; RTL2832      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_3EF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3DC0&MI_00            ; RTL2836          AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3DD0&MI_00            ; RTL2836          AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3DE0&MI_00            ; RTL2836      W/O AVS     FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DE0&MI_01            ;  								HID BY USER 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3DF0&MI_00            ; RTL2836      W/O AVS W/O FM
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3DF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DC9&MI_00            ; RTL2836          AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DD9&MI_00            ; RTL2836          AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DE9&MI_00            ; RTL2836      W/O AVS     FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_1DF9&MI_00            ; RTL2836      W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DTMB%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_1DF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3CC0&MI_00            ; DRXJ             AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CC0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CC6&MI_01            ; 								HID RC6 (MICROSOFT)
 
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3CD0&MI_00            ; DRXJ             AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CD0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3CE0&MI_00            ; DRXJ         W/O AVS     FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CE0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3CF0&MI_00            ; DRXJ         W/O AVS W/O FM
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CF0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3CC9&MI_00            ; DRXJ             AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3CD9&MI_00            ; DRXJ             AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3CE9&MI_00            ; DRXJ         W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3CF9&MI_00            ; DRXJ         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC%                       =         POLARIS.RDU253S,   USB\VID_1164&PID_3CF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3BC0&MI_00            ; DRXK             AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BC0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3BD0&MI_00            ; DRXK             AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3BE0&MI_00            ; DRXK         W/O AVS     FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BE0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BE6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3BF0&MI_00            ; DRXK         W/O AVS W/O FM
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3BC9&MI_00            ; DRXK             AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BC9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3BD9&MI_00            ; DRXK             AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3BE9&MI_00            ; DRXK         W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3BF9&MI_00            ; DRXK         W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBTC%                      =         POLARIS.RDU253S,   USB\VID_1164&PID_3BF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3AC0&MI_00            ; DVBT/ATSC        AVS     FM
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AC0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AC6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3AD0&MI_00            ; DVBT/ATSC        AVS W/O FM
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AD0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AD6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3AE0&MI_00            ; DVBT/ATSC    W/O AVS     FM
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AE0&MI_01            ; 								HID BY USER
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AE6&MI_01            ; 								HID RC6 (MICROSOFT)
 
%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_3AF0&MI_00            ; DVBT/ATSC    W/O AVS W/O FM
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AF0&MI_01            ;  								HID BY USER
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AF6&MI_01            ; 								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3AC9&MI_00            ; DVBT/ATSC        AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AC9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3AD9&MI_00            ; DVBT/ATSC        AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC.NL                =         POLARIS.RDU253S,   USB\VID_1164&PID_3AD9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3AE9&MI_00            ; DVBT/ATSC    W/O AVS     FM	W/O HID 
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AE9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_3AF9&MI_00            ; DVBT/ATSC    W/O AVS W/O FM	W/O HID 
%CXPOLARIS.DVBT.ATSC.NL%               =         POLARIS.RDU253S,   USB\VID_1164&PID_3AF9&MI_01            ; 

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_39C0&MI_00            ; LGDT3305         AVS     FM
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39C0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39C6&MI_01            ;								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_39D0&MI_00            ; LGDT3305         AVS W/O FM
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39D0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39D6&MI_01            ;								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_39E0&MI_00            ; LGDT3305     W/O AVS     FM
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39E0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39E6&MI_01            ;								HID RC6 (MICROSOFT)

%CXPOLARIS.HID%                        =         POLARIS.CIR,       USB\VID_1164&PID_39F0&MI_00            ; LGDT3305     W/O AVS W/O FM
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39F0&MI_01            ;  								HID BY USER
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39F6&MI_01            ;								HID RC6 (MICROSOFT)

%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_39C9&MI_00            ; LGDT3305         AVS     FM	W/O HID 
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39C9&MI_01            ; 
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_39D9&MI_00            ; LGDT3305         AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39D9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_39E9&MI_00            ; LGDT3305     W/O AVS     FM	W/O HID 
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39E9&MI_01            ;
%CXPOLARIS.CIR%                        =         POLARIS.CIR.DUMMY, USB\VID_1164&PID_39F9&MI_00            ; LGDT3305     W/O AVS W/O FM	W/O HID 
%CXPOLARIS.ATSC.NL%                    =         POLARIS.RDU253S,   USB\VID_1164&PID_39F9&MI_01            ; 

[POLARIS.RDU253S]
Include                                =         ks.inf, kscaptur.inf,ksfilter.inf, wdmaudio.inf, bda.inf
Needs                                  =         KS.Registration, KSCAPTUR.Registration,MSPCLOCK.Installation, WDMAUDIO.Registration, BDA.Registration, bda.Installation
AddReg                                 =         POLARIS.AddReg,POLARISVID.AddReg,CXDVBT.AddReg, RDU253S.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers,DSFilters.CopyFiles
RegisterDlls                           =         DSFilters.RegDLL    

[POLARIS.RDU253S.NT]
Include                                =         ks.inf, kscaptur.inf,ksfilter.inf, wdmaudio.inf, bda.inf
Needs                                  =         KS.Registration, KSCAPTUR.Registration.NT,MSPCLOCK.Installation, WDMAUDIO.Registration, BDA.Registration, bda.Installation.NT
AddReg                                 =         POLARIS.AddReg,PolarisVID.AddReg,CXDVBT.AddReg, RDU253S.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers,DSFilters.CopyFiles
RegisterDlls                           =         DSFilters.RegDLL  

[POLARIS.CAPTURE]
Include                                =         ks.inf, kscaptur.inf,ksfilter.inf, wdmaudio.inf, bda.inf
Needs                                  =         KS.Registration, KSCAPTUR.Registration,MSPCLOCK.Installation, WDMAUDIO.Registration, BDA.Registration, bda.Installation
AddReg                                 =         POLARIS.AddReg,POLARISVID.AddReg,CXDVBT.AddReg, RDU253S.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers,DSFilters.CopyFiles
RegisterDlls                           =         DSFilters.RegDLL    

[POLARIS.CAPTURE.NT]
Include                                =         ks.inf, kscaptur.inf,ksfilter.inf, wdmaudio.inf, bda.inf
Needs                                  =         KS.Registration, KSCAPTUR.Registration.NT,MSPCLOCK.Installation, WDMAUDIO.Registration, BDA.Registration, bda.Installation.NT
AddReg                                 =         POLARIS.AddReg,PolarisVID.AddReg,CXDVBT.AddReg, RDU253S.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers,DSFilters.CopyFiles
RegisterDlls                           =         DSFilters.RegDLL  

[POLARIS.CIR]
AddReg                                 =         CXIR.AddReg,CX_IR.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers

[POLARIS.CIR.NT]
AddReg                                 =         CXIR.AddReg,CX_IR.AddReg
CopyFiles                              =         CXPOLARIS.CopyDrivers

[POLARIS.CIR.DUMMY]

[POLARIS.CIR.DUMMY.NT]

[DestinationDirs]
CXPOLARIS.CopyDrivers                  =         10,system32\drivers
DSFilters.CopyFiles                    =         11

[CXPOLARIS.CopyDrivers]
cxRDU253S.sys
cxPolarIR.sys
merlinD.rom

[DSFilters.CopyFiles]
cpnotify.ax

[DSFilters.RegDLL]
11,,cpnotify.ax,1

[PolarisVID.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cxRDU253S.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,%MediaCategories%\%POLARIS_GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%
HKLM,%MediaCategories%\%POLARIS_GUID.PINNAME_AUDIO_OUT%,Name,,%PinName.AnalogAudioOut%

HKLM,System\CurrentControlSet\Control\MediaInterfaces\{868de3d7-1ed1-4698-af07-0a4b57662572},,,"Notify Copy Protect Filter"
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{868de3d7-1ed1-4698-af07-0a4b57662572},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

;Wave in audio device registration
HKR,Drivers,SubClasses,,"wave"
HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%PRODUCT.ANALOGX.AUDIO.NAME%
HKR,"DriverData","CpMethod",0x00010001, 0xFE, 0x00, 0x00, 0x00

[POLARIS.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","EnableHANCAudioOut",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","gpio_pin_status_mask",0x00010001, 0x4001000
HKR,"DriverData","ctrl_pin_status_mask",0x00010001, 0xFFFFFFC4

;---Crossbar registry values---
; Note: For each pin on the crossbar, specify the following:
; (1) Pin type
;     0 - SVIDEO
;     1 - Tuner
;     2 - Composite
;     3 - audio tuner in
;     4 - audio line in
;     7 - YUV
; (2) InputMux - input mux to use for the selected pin
; (3) RelatedPinIndex
;-------------------------------------------------------------------

;Pin 0 - Tuner In
; Input Mux       : VIN2_1 for Tuner input from Nxp18271
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite in
; Input Mux       : VIN2_1 for Composite
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video in
; Input Mux       : VIN1_1 for Luma, VIN1_2 for Chroma
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x01,0x01,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line in
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","GpioMask",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","GpioSettings",0x00010001, 0x00,0x00,0x00,0x00

HKR,"DriverData","VideoInputPin",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData","AudioInputPin",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

[RDU253S.AddReg]
HKR,"DriverData","BoardType",0x00010001, 0x0A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerType",0x00010001, 0x28, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC0, 0x00, 0x00, 0x00
HKR,"DriverData","I2CSpeed",0x00010001, 0x2, 0x00, 0x00, 0x00
HKR,"DriverData","Enable_SW_Encoder",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","NoOfTuners",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCategory",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit", 0x00010001, 0x05, 0x00, 0x00, 0x00
HKR,"DriverData","XC_GPIO_I2C_SCL", 0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","XC_GPIO_I2C_SDA", 0x00010001, 0x1B, 0x00, 0x00, 0x00
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CMaster",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CMaster",0x00010001, 0x03, 0x00, 0x00, 0x00
HKR,"DriverData","Audio_Volume",0x00010001, 0x16, 0x00, 0x00, 0x00

[CXDVBT.AddReg]
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%TSPinID%,Name,,%TSPinName%

[CXIR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,cxPolarIR.sys

[CX_IR.AddReg]
HKR,"DriverData","IR_Command_Table",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","IR_PROTOCOL",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","IR_PROTOCOL_MODE",0x00010001, 0x0c, 0x00, 0x00, 0x00

HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"IRType",0x10001,2
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"0",0x00001,0d,01,00,27
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"1",0x00001,04,01,00,1e
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"2",0x00001,05,01,00,1f
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"3",0x00001,06,01,00,20
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"4",0x00001,07,01,00,21
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"5",0x00001,08,01,00,22
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"6",0x00001,09,01,00,23
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"7",0x00001,0a,01,00,24
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"8",0x00001,1b,01,00,25
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"9",0x00001,1f,01,00,26
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"10",0x00001,03,01,00,56
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"11",0x00001,1e,01,00,57
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"12",0x00001,01,01,00,41
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"13",0x00001,02,01,00,42
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"14",0x00001,1a,01,00,43
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"15",0x00001,12,11,05,45
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"16",0x00001,0c,11,04,28
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"17",0x00001,0e,01,00,44
HKLM,System\CurrentControlSet\SERVICES\POLARIS_CIR,"KeyMapNumber",0x10001,18

[POLARIS.RDU253S.Interfaces]
AddInterface                =     %KSCATEGORY_TVTUNER%,                %ANALOG.TVTUNER.FILTER.GUID%,    CX23102.Tvtuner.Interface
AddInterface                =     %KSCATEGORY_TVAUDIO%,                %ANALOG.TVAUDIO.FILTER.GUID%,    CX23102.TvAudio.Interface
AddInterface                =     %KSCATEGORY_CROSSBAR%,               %ANALOG.CROSSBAR.FILTER.GUID%,   CX23102.Crossbar.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.CAPTUER.FILTER.GUID%,    CX23102.Capture.Interface
;AddInterface               =     %KSCATEGORY_AUDIO%,                  %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface

AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.A%,   CX23102.BDATuner.InterfaceA
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.B%,   CX23102.BDATuner.InterfaceB
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.C%,   CX23102.BDATuner.InterfaceC
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.A%, CX23102.BDACapture.InterfaceA
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.B%, CX23102.BDACapture.InterfaceB
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.C%, CX23102.BDACapture.InterfaceC

[POLARIS.RDU253S.NT.Interfaces]
AddInterface                =     %KSCATEGORY_TVTUNER%,                %ANALOG.TVTUNER.FILTER.GUID%,    CX23102.Tvtuner.Interface
AddInterface                =     %KSCATEGORY_TVAUDIO%,                %ANALOG.TVAUDIO.FILTER.GUID%,    CX23102.TvAudio.Interface
AddInterface                =     %KSCATEGORY_CROSSBAR%,               %ANALOG.CROSSBAR.FILTER.GUID%,   CX23102.Crossbar.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.CAPTUER.FILTER.GUID%,    CX23102.Capture.Interface
;AddInterface               =     %KSCATEGORY_AUDIO%,                  %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface

AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.A%,   CX23102.BDATuner.InterfaceA
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.B%,   CX23102.BDATuner.InterfaceB
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.C%,   CX23102.BDATuner.InterfaceC
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.A%, CX23102.BDACapture.InterfaceA
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.B%, CX23102.BDACapture.InterfaceB
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.C%, CX23102.BDACapture.InterfaceC

[POLARIS.CAPTURE.Interfaces]
AddInterface                =     %KSCATEGORY_TVTUNER%,                %ANALOG.TVTUNER.FILTER.GUID%,    CX23102.Tvtuner.Interface
AddInterface                =     %KSCATEGORY_TVAUDIO%,                %ANALOG.TVAUDIO.FILTER.GUID%,    CX23102.TvAudio.Interface
AddInterface                =     %KSCATEGORY_CROSSBAR%,               %ANALOG.CROSSBAR.FILTER.GUID%,   CX23102.Crossbar.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.CAPTUER.FILTER.GUID%,    CX23102.Capture.Interface
AddInterface                =     %KSCATEGORY_AUDIO%,                  %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface

AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.A%,   CX23102.BDATuner.InterfaceA
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.B%,   CX23102.BDATuner.InterfaceB
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.C%,   CX23102.BDATuner.InterfaceC
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.A%, CX23102.BDACapture.InterfaceA
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.B%, CX23102.BDACapture.InterfaceB
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.C%, CX23102.BDACapture.InterfaceC

[POLARIS.CAPTURE.NT.Interfaces]
AddInterface                =     %KSCATEGORY_TVTUNER%,                %ANALOG.TVTUNER.FILTER.GUID%,    CX23102.Tvtuner.Interface
AddInterface                =     %KSCATEGORY_TVAUDIO%,                %ANALOG.TVAUDIO.FILTER.GUID%,    CX23102.TvAudio.Interface
AddInterface                =     %KSCATEGORY_CROSSBAR%,               %ANALOG.CROSSBAR.FILTER.GUID%,   CX23102.Crossbar.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.CAPTUER.FILTER.GUID%,    CX23102.Capture.Interface
AddInterface                =     %KSCATEGORY_AUDIO%,                  %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface
AddInterface                =     %KSCATEGORY_CAPTURE%,                %ANALOG.AUDIO.FILTER.GUID%,      CX23102.Audio.Interface

AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.A%,   CX23102.BDATuner.InterfaceA
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.B%,   CX23102.BDATuner.InterfaceB
AddInterface                =     %KSCATEGORY_BDATUNER%,               %DIGITAL.TUNER.FILGER.GUID.C%,   CX23102.BDATuner.InterfaceC
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.A%, CX23102.BDACapture.InterfaceA
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.B%, CX23102.BDACapture.InterfaceB
AddInterface                =     %KSCATEGORY_BDA_RECEIVER_COMPONENT%, %DIGITAL.CAPTURE.FILGER.GUID.C%, CX23102.BDACapture.InterfaceC

[CX23102.Tvtuner.Interface]
AddReg = CX23102.Tvtuner.Interface.AddReg

[CX23102.Tvtuner.Interface.AddReg]
HKR,,CLSID,,%KSTVTUNE.CLSID%
HKR,,FriendlyName,,%PRODUCT.ANALOGX.TVTUNER.NAME%
HKR,,TunerInstanceID,0x00010001,10

[CX23102.TvAudio.Interface]
AddReg=CX23102.TvAudio.Interface.AddReg

[CX23102.TvAudio.Interface.AddReg]
HKR,,CLSID,,%KSTVAUDIO.CLSID%
HKR,,FriendlyName,,%PRODUCT.ANALOGX.TVAUDIO.NAME%

[CX23102.Crossbar.Interface]
AddReg=CX23102.Crossbar.Interface.AddReg

[CX23102.Crossbar.Interface.AddReg]
HKR,,CLSID,,%KSXBAR.CLSID%
HKR,,FriendlyName,,%PRODUCT.ANALOGX.CROSSBAR.NAME%

[CX23102.Capture.Interface]
AddReg=CX23102.Capture.Interface.AddReg
AddReg=POLARIS_RDU253S_DESCRIPTION.AddReg

[CX23102.Capture.Interface.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID%      
HKR,,FriendlyName,,%PRODUCT.ANALOGX.CAPTUER.NAME%

[POLARIS_RDU253S_DESCRIPTION.AddReg]
HKR,,Description,,%CXPOLARIS.DeviceDesc%

[CX23102.Audio.Interface]
AddReg=CX23102.Audio.Interface.AddReg

[CX23102.Audio.Interface.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID%      
HKR,,FriendlyName,,%PRODUCT.ANALOGX.AUDIO.NAME%

[CX23102.BDATuner.InterfaceA]
AddReg = CX23102.BDATuner.InterfaceA.AddReg

[CX23102.BDATuner.InterfaceA.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID%
HKR,,FriendlyName,,%PRODUCT.DIGITAL.TUNER.A.NAME%
HKR,,TunerInstanceID,0x00010001,10

[CX23102.BDATuner.InterfaceB]
AddReg = CX23102.BDATuner.InterfaceB.AddReg

[CX23102.BDATuner.InterfaceB.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID%
HKR,,FriendlyName,,%PRODUCT.DIGITAL.TUNER.B.NAME%
HKR,,TunerInstanceID,0x00010001,10

[CX23102.BDATuner.InterfaceC]
AddReg = CX23102.BDATuner.InterfaceC.AddReg

[CX23102.BDATuner.InterfaceC.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID%
HKR,,FriendlyName,,%PRODUCT.DIGITAL.TUNER.C.NAME%
HKR,,TunerInstanceID,0x00010001,10

[CX23102.BDACapture.InterfaceA]
AddReg=CX23102.BDACapture.InterfaceA.AddReg

[CX23102.BDACapture.InterfaceA.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID% 
HKR,,FriendlyName,,%PRODUCT.DIGITAL.CAPTUER.A.NAME%

[CX23102.BDACapture.InterfaceB]
AddReg=CX23102.BDACapture.InterfaceB.AddReg

[CX23102.BDACapture.InterfaceB.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID% 
HKR,,FriendlyName,,%PRODUCT.DIGITAL.CAPTUER.B.NAME%

[CX23102.BDACapture.InterfaceC]
AddReg=CX23102.BDACapture.InterfaceC.AddReg

[CX23102.BDACapture.InterfaceC.AddReg]
HKR,,CLSID,,%KSPROXY.CLSID% 
HKR,,FriendlyName,,%PRODUCT.DIGITAL.CAPTUER.C.NAME%

[POLARIS.RDU253S.Services]
AddService                                  = CXPOLARIS,2,PolarisVID.RDU253S.ServiceInstall

[POLARIS.RDU253S.NT.Services]
AddService                                  = CXPOLARIS,2,PolarisVID.RDU253S.ServiceInstall

[POLARIS.CAPTURE.Services]
AddService                                  = CXPOLARIS,2,PolarisVID.RDU253S.ServiceInstall

[POLARIS.CAPTURE.NT.Services]
AddService                                  = CXPOLARIS,2,PolarisVID.RDU253S.ServiceInstall

[POLARIS.CIR.Services]
AddService                                  = CXIR,2,POLARIS.CIR.ServiceInstall

[POLARIS.CIR.NT.Services]
AddService                                  = CXIR,2,POLARIS.CIR.ServiceInstall

[POLARIS.CIR.DUMMY.Services]
AddService                                  = ,2               ; null service install

[POLARIS.CIR.DUMMY.NT.Services]
AddService                                  = ,2               ; null service install

[POLARIS.CIR.ServiceInstall]
DisplayName                                 = %CX_IR.DeviceDesc%
ServiceType                                 = 1
StartType                                   = 2
ErrorControl                                = 1
ServiceBinary                               = %10%\system32\drivers\cxPolarIR.sys

[PolarisVID.RDU253S.ServiceInstall]
DisplayName                                 = %CXPOLARIS.DeviceDesc%
ServiceType                                 = 1
StartType                                   = 3
ErrorControl                                = 1
ServiceBinary                               = %10%\system32\drivers\cxRDU253S.sys
;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
CXPOLARIS.DeviceDesc                        = "YUAN Polaris Hybrid TV AVS Video Capture"
CX_IR.DeviceDesc                            = "YUAN Polaris IR Transceiver"
Company                                     = "YUAN High-Tech Development Co., Ltd"

CXPOLARIS.ANALOG                            = "YUAN MC182A/PD182A Analog TV AVS Video Capture"
CXPOLARIS.DTMB                              = "YUAN MC182/PD182 DTMB Hybrid TV AVS Video Capture"
CXPOLARIS.DVBT                              = "YUAN MC782ML/PD782S DVB-T Hybrid TV AVS Video Capture"
CXPOLARIS.ATSC                              = "YUAN MC582ML/PD582 ATSC/QAM Hybrid TV AVS Video Capture"
CXPOLARIS.DVBT.NL                           = "YUAN MC782NL/PD782SN DVB-T Hybrid TV AVS Video Capture"
CXPOLARIS.ATSC.NL                           = "YUAN MC582NL ATSC/QAM Hybrid TV AVS Video Capture"
CXPOLARIS.DVBTC                             = "YUAN MC782/PD782 DVB-T/DVB-C Hybrid TV AVS Video Capture"
CXPOLARIS.DVBT.ATSC                         = "YUAN MC982ML DVB-T/ATSC/QAM Hybrid TV AVS Video Capture"
CXPOLARIS.DVBT.ATSC.NL                      = "YUAN MC982NL DVB-T/ATSC/QAM Hybrid TV AVS Video Capture"
CXPOLARIS.CAPTURE                           = "YUAN AVS Video Capture"
CXPOLARIS.CIR                               = "YUAN HID Infrared Remote Receiver (Dummy)"
CXPOLARIS.HID                               = "YUAN HID Infrared Remote Receiver"

PRODUCT.ANALOGX.CAPTUER.NAME                = "Conexant Polaris Video Capture"
PRODUCT.ANALOGX.TVAUDIO.NAME                = "Conexant Polaris TvAudio"
PRODUCT.ANALOGX.TVTUNER.NAME                = "Conexant Polaris Tuner"
PRODUCT.ANALOGX.AUDIO.NAME                  = "Conexant Polaris Audio Capture"
PRODUCT.ANALOGX.CROSSBAR.NAME               = "Conexant Polaris Crossbar"
PRODUCT.DIGITAL.TUNER.A.NAME                = "Conexant Polaris BDA Tuner"
PRODUCT.DIGITAL.TUNER.B.NAME                = "Conexant Polaris BDA Tuner (QAM)"
PRODUCT.DIGITAL.TUNER.C.NAME                = "Conexant Polaris BDA Tuner DVB-T"
PRODUCT.DIGITAL.CAPTUER.A.NAME              = "Conexant Polaris AVStream TS Capture"
PRODUCT.DIGITAL.CAPTUER.B.NAME              = "Conexant Polaris AVStream TS Capture (QAM)"
PRODUCT.DIGITAL.CAPTUER.C.NAME              = "Conexant Polaris AVStream TS Capture DVB-T"

ANALOG.CAPTUER.FILTER.GUID                  = "{9B365890-165F-11D0-A195-0020AFD156E4}"
ANALOG.TVAUDIO.FILTER.GUID                  = "{D8D86791-A570-4a10-8457-08C957E90ECD}"
ANALOG.CROSSBAR.FILTER.GUID                 = "{47B00748-34A2-4000-A892-BA2ABF2E2BE4}"
ANALOG.TVTUNER.FILTER.GUID                  = "{F7CCD5C2-8766-4401-BF9D-ECF5FE0A07C0}"
ANALOG.AUDIO.FILTER.GUID                    = "{5EAF914D-2212-4034-8C4C-02CAFD15D68A}"

KSCATEGORY_AUDIO                            = "{33D9A762-90C8-11D0-BD43-00A0C911CE86}"
;KSCATEGORY_AUDIO                           = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}" ;qcap interface
KSCATEGORY_CAPTURE                          = "{65e8773d-8f56-11d0-a3b9-00a0c9223196}"
KSCATEGORY_TVAUDIO                          = "{a799a802-a46d-11d0-a18c-00a02401dcd4}"
KSCATEGORY_TVTUNER                          = "{a799a800-a46d-11d0-a18c-00a02401dcd4}"
KSCATEGORY_CROSSBAR                         = "{a799a801-a46d-11d0-a18c-00a02401dcd4}"
KSCATEGORY_BDATUNER                         = "{71985F48-1CA1-11d3-9CC8-00C04F7971E0}"
KSCATEGORY_BDA_RECEIVER_COMPONENT           = "{FD0A5AF4-B41D-11d2-9C95-00C04F7971E0}"

KSTVTUNE.CLSID                              = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"
KSTVAUDIO.CLSID                             = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSXBAR.CLSID                                = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSPROXY.CLSID                               = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

DIGITAL.TUNER.FILGER.GUID.A                 = "{E01E1072-3DF3-4C23-B99F-6A27A7CC7CD2}"
DIGITAL.TUNER.FILGER.GUID.B                 = "{E01E1072-3DF3-4C23-B99F-6A27A7CC7ED2}"  ; QAM GUID
DIGITAL.TUNER.FILGER.GUID.C                 = "{E01E1072-3DF3-4C23-B99F-6A27A7CC7AD2}"  ; DVB-T GUID
DIGITAL.CAPTURE.FILGER.GUID.A               = "{452660BD-3B39-4e34-9B97-3D3BC054AF5D}"
DIGITAL.CAPTURE.FILGER.GUID.B               = "{452660BD-3B39-4e34-9B97-3D3BC054AD5D}"  ; QAM GUID
DIGITAL.CAPTURE.FILGER.GUID.C               = "{452660BD-3B39-4e34-9B97-3D3BC054AB5D}"  ; DVB-T GUID

PinName.AnalogAudioOut                      = "Audio Out"
Pin.p2AnalogAudioIn                         = "Analog Audio In"
TSPinName                                   = "TS Out"
POLARIS_GUID.PINNAME_ANALOG_AUDIO_IN        = "{3E2D189F-B15C-4447-96F1-BD1D64FB99BA}"
POLARIS_GUID.PINNAME_AUDIO_OUT              = "{13FFFECC-3C46-4e52-8B07-4ED850E5FB49}"
GUID.POLARIS_VERSION_INFORMATION_PROPERTIES = "{2038EEA5-AE84-4a00-B174-9673AB35F1DC}"
GUID.DriverVersion_Properties               = "{1979C7E7-FB3B-42ff-B070-0D8F49A1A42D}"
MediaCategories                             = "SYSTEM\CurrentControlSet\Control\MediaCategories"
MediaSets                                   = "System\CurrentControlSet\Control\MediaSets"
MediaInterfaces                             = "System\CurrentControlSet\Control\MediaInterfaces"
BdaSWTuner.DeviceId                         = "{828B00F0-9A04-4692-8573-535B05DFF3F4}"
TSPinID                                     = "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
