; Windows Modem Setup File
; Copyright (c) 1993-2006 Microsoft Corporation
; Manufacturer: Sony Ericsson

[Version]
CatalogFile=EEXX.cat
Signature="$Windows NT$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%ModemProvider%
DriverVer=11/10/2006,4.0.0.66

[DestinationDirs]
DefaultDestDirs			= 11
Drv.Copy=12

[Manufacturer]
%ModemProvider%=GPRS_Modems

[GPRS_Modems]
%USB2132.Modem% = EDGE.Modem, USB\VID_0FCE&PID_D019

[ControlFlags]
ExcludeFromSelect = *

[WM_Device_LowerFilter]
HKR,,LowerFilters,0x00010000,SEMWModem

[WM_Device_Service_Inst]
DisplayName    = %ModemProvider% SEMWModem
ServiceType    = 1
StartType      = 3   
ErrorControl   = 1
ServiceBinary  = %12%\EEXX.sys
AddReg		   = Reg.DevName

[Strings]
TCPWindowSizeDesc	= "TCP Window Size"
MTUDesc				= "MTU Size"
LegacyDeviceName			="GC75"
USB2132.Modem="Sony Ericsson VDC EGPRS Modem"
USB2132MaxLinkSpeed="2144"
Version = "4.0.0.66"
Disk1Name			="Sony Ericsson WWAN Installation Disk "
DeviceName			="GCXX"
NicDeviceID			="GCXX\GPRS_NIC_REV01"
SCDeviceID			="GCXX\SIM_SC"
ModemProvider="Sony Ericsson"
FullProductName="Sony Ericsson Wireless Modem"
ShortProductName="WModem"

[Drv.Copy]
EEXX.sys

; Driver Settings and Configuration
[Reg.MdmCommon]
HKR,%USB2132.Modem%,xKeepStateOnStop,1,04
HKR,%USB2132.Modem%,USBV24Emulation,1,00
HKR,%USB2132.Modem%,MaxLinkSpeed,,%USB2132MaxLinkSpeed%
HKR,%USB2132.Modem%,xMuxFrameSize,1,7F
HKR,%USB2132.Modem%,xStartHoldTime,1,E8,03,00,00
HKR,%USB2132.Modem%,xFuncRetryCount,1,02
HKR,%USB2132.Modem%,xMuxRetryCount,1,01
HKR,%USB2132.Modem%,xIdleInterval,1,E8,03,00,00

[Reg.MdmPort]
HKR,,DevLoader,,*vcomm
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
HKR, Init, 1,, "AT<cr>"
HKR,, DeviceType, 1, 03

[Reg.DevName]
HKR,Parameters,LegacyDeviceName,,%LegacyDeviceName%
HKR,Parameters,DeviceName,,%DeviceName%
HKR,Parameters,NicDeviceID,,%NicDeviceID%
HKR,Parameters,SCDeviceID,,%SCDeviceID%

; Modem Commands and Responses
[Reg.MdmRsp]
HKR, Fax, HardwareFlowControl,, "1"
HKR, Fax, FixModemClass,,"2.0"
HKR, Init, 1,, "AT<cr>"
HKR, Init, 2,, "AT&F&D2&C1E0V1S0=0<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Answer, 1,, "ATA<cr>"
HKR, Hangup, 1,, "ATH<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, FlowControl_Off,,"+IFC=0,0"
HKR, Settings, FlowControl_Hard,,"+IFC=2,2"
HKR, Settings, FlowControl_Soft,,"+IFC=1,1"
HKR, Settings, ErrorControl_Forced,,"+ER=3;+ES=4,2,6"
HKR, Settings, ErrorControl_Off,,"+ER=0;+ES=1,0,1"
HKR, Settings, ErrorControl_On,,"+ER=3;+ES=4,0,2"
HKR, Settings, Compression_Off,,"+DR=0;+DS=0"
HKR, Settings, Compression_On,,"+DR=1;+DS=3,0,2048,32"
;HKR,Settings,CallSetupFailTimer,,"S7=<#>"
;HKR,Settings,InactivityTimeout,,"S10=<#>"
HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>FAX<cr><lf>",         1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DATA<cr><lf>",        1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>VOICE<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "1<cr>",       1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "<cr><lf>+DR: NONE<cr><lf>",                1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+DR: V42B<cr><lf>",                1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+DR: V42B RD<cr><lf>",             1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+DR: V42B TD<cr><lf>",             1, 01, 01, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+ER: NONE<cr><lf>",                1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+ER: LAPM<cr><lf>",                1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>+ER: ALT<cr><lf>",                 1, 01, 02, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",            1, 02, 00, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/REL<cr><lf>",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 9600/MNP<cr><lf>",        1, 02, 02, 80,25,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",           1, 02, 00, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/REL<cr><lf>",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 14400/MNP<cr><lf>",       1, 02, 02, 40,38,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",           1, 02, 00, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/REL<cr><lf>",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 19200/MNP<cr><lf>",       1, 02, 02, 00,4B,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",           1, 02, 00, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/REL<cr><lf>",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 28800/MNP<cr><lf>",       1, 02, 02, 80,70,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",           1, 02, 00, 00,96,00,00, 00,00,00,00 
HKR, Responses, "<cr><lf>CONNECT 38400/REL<cr><lf>",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 38400/MNP<cr><lf>",       1, 02, 02, 00,96,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 43200<cr><lf>",           1, 02, 00, C0,A8,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 43200/REL<cr><lf>",       1, 02, 02, C0,A8,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 43200/MNP<cr><lf>",       1, 02, 02, C0,A8,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",           1, 02, 00, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/REL<cr><lf>",       1, 02, 02, 00,E1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT 57600/MNP<cr><lf>",       1, 02, 02, 00,E1,00,00, 00,00,00,00

[Reg.LegRsp]
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,C2,01,00, 60,D1,00,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 60,D1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/REL<cr><lf>",             1, 02, 02, 60,D1,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/MNP<cr><lf>",             1, 02, 02, 60,D1,00,00, 00,00,00,00

[Reg.EdgRsp]
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,10,0E,00, 80,45,03,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 80,45,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/REL<cr><lf>",             1, 02, 02, 80,45,03,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/MNP<cr><lf>",             1, 02, 02, 80,45,03,00, 00,00,00,00

[Reg.UMTRsp]
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,10,0E,00, 00,DC,05,00
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",                 1, 02, 00, 00,DC,05,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/REL<cr><lf>",             1, 02, 02, 00,DC,05,00, 00,00,00,00
HKR, Responses, "<cr><lf>CONNECT/MNP<cr><lf>",             1, 02, 02, 00,DC,05,00, 00,00,00,00

[SourceDisksNames]
1=%Disk1Name%,,

[SourceDisksFiles]
EEXX.sys = 1

[GPRS.Modem.NT]
CopyFiles=Drv.Copy
AddReg=Reg.MdmCommon, Reg.MdmPort, Reg.MdmRsp, Reg.LegRsp

[GPRS.Modem.NT.Services]
AddService = SEMWModem, 0x00000000, WM_Device_Service_Inst

[GPRS.Modem.NT.HW]
AddReg=WM_Device_LowerFilter

[EDGE.Modem.NT]
CopyFiles=Drv.Copy
AddReg=Reg.MdmCommon, Reg.MdmPort, Reg.MdmRsp, Reg.EdgRsp

[EDGE.Modem.NT.Services]
AddService = SEMWModem, 0x00000000, WM_Device_Service_Inst

[EDGE.Modem.NT.HW]
AddReg=WM_Device_LowerFilter

[UMTS.Modem.NT]
CopyFiles=Drv.Copy
AddReg=Reg.MdmCommon, Reg.MdmPort, Reg.MdmRsp, Reg.UMTRsp

[UMTS.Modem.NT.Services]
AddService = SEMWModem, 0x00000000, WM_Device_Service_Inst

[UMTS.Modem.NT.HW]
AddReg=WM_Device_LowerFilter
