;
; CAB200.INF
;

[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGuid={36FC9E60-C465-11CF-8056-444553540000}
Provider=%PRODUCT_COMPANY%
CatalogFile=CAB200.CAT
DriverVer=06/08/2007,1.1.0.0

[Manufacturer]
%PRODUCT_COMPANY%=TEAC, NTx86, NTamd64

[TEAC]
%USB\VID_0644&PID_0201.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0201
%USB\VID_0644&PID_0200.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0200

[TEAC.NTamd64]
%USB\VID_0644&PID_0201.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0201
%USB\VID_0644&PID_0200.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0200

[TEAC.NTx86]
%USB\VID_0644&PID_0201.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0201
%USB\VID_0644&PID_0200.DeviceDesc% = TEAC_BULK, USB\VID_0644&PID_0200

[TEAC_BULK.NT]
Include = usbstor.inf
Needs   = USBSTOR_BULK.NT
AddReg=USBSTOR_BULK.AddReg, USBSTOR_NR.AddReg, TEAC.AddReg
CopyFiles=@TEACico2.dll

[TEAC_BULK.NT.Services]
Include = usbstor.inf
Needs   = USBSTOR_BULK.NT.Services

[TEAC.AddReg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_CF,Icons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,0" 
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_CF,Label,0x00000000,"Compact Flash Drive"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_CF,NoMediaIcons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,1"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_XDSM,Icons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,2" 
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_XDSM,Label,0x00000000,"xD/SM Drive"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_XDSM,NoMediaIcons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,3"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_MS,Icons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,4" 
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_MS,Label,0x00000000,"Memory Stick Drive"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_MS,NoMediaIcons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,5"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_SD,Icons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,6" 
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_SD,Label,0x00000000,"SD Card Drive"
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Explorer\AutoplayHandlers\DeviceGroups\TEAC_SD,NoMediaIcons,0x00010000,"%SystemRoot%\system32\TEACico2.dll,7"

HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskTEAC____USB___HS-CF_Card,DeviceGroup,0x00000000,"TEAC_CF"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskTEAC____USB___HS-xD/SM__,DeviceGroup,0x00000000,"TEAC_XDSM"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskTEAC____USB___HS-MS_Card,DeviceGroup,0x00000000,"TEAC_MS"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskTEAC____USB___HS-SD_Card,DeviceGroup,0x00000000,"TEAC_SD"

HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskDELL____USB___HS-CF_Card,DeviceGroup,0x00000000,"TEAC_CF"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskDELL____USB___HS-xD/SM__,DeviceGroup,0x00000000,"TEAC_XDSM"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskDELL____USB___HS-MS_Card,DeviceGroup,0x00000000,"TEAC_MS"
HKLM,SOFTWARE\Microsoft\Windows NT\CurrentVersion\PerHwIdStorage\USBSTOR#DiskDELL____USB___HS-SD_Card,DeviceGroup,0x00000000,"TEAC_SD"

[SourceDisksNames]
1= %PRODUCT_SERVICE% %SOURCEDISK_DESC%

[DestinationDirs]
DefaultDestDir = 11 ;Windows System directory
 
[SourceDisksFiles]
TEACico2.dll = 1,,,,,

[Strings]
PRODUCT_COMPANY = "TEAC"
PRODUCT_SERVICE = "USB Card Reader Driver"
SOURCEDISK_DESC = "Source Disk #1"
USB\VID_0644&PID_0201.DeviceDesc = "CAB-200"
USB\VID_0644&PID_0200.DeviceDesc = "CA-200"
