;//////////////////////////////////////////////////
;VP5083 dirver-------------audio inf
///////////////////////////////////////////////////
[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Twinhan"
DriverVer=07/25/2005,0.0.1.1


[Manufacturer]
"Twinhan"=Twinhan

[SourceDisksNames]
1="Twinhan VP5083 Drivers",,,""

[SourceDisksFiles]
TV5083aud.sys=1

[Twinhan]
%CX23880.DeviceDesc%=AUD,  PCI\VEN_14F1&DEV_8801&SUBSYS_00201822

[AUD]
Include=    ks.inf, kscaptur.inf, bda.inf
Needs=      KS.Registration
AddReg=     CX880.AddReg,AUD.AddReg
CopyFiles=  CX880.CopyDrivers


[DestinationDirs]
CX880.CopyDrivers=10,system32\drivers

[CX880.CopyDrivers]
TV5083aud.sys

[CX880.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,TV5083aud.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\%AudioPinID%,Display,1, 00,00,00,00
HKLM,System\CurrentControlSet\Control\MediaCategories\%AudioPinID%,Name,,%AudioPinName%

;
; Driver Configuration Registry Entries
;

[AUD.AddReg]
; Default to tuner input
HKR,"DriverData","InputSelect",0x00010001,   0x00,0x00,0x00,0x00

; 48 KHz operation
HKR,"DriverData","SampleRate" ,0x00010001,   0x80,0xBB,0x00,0x00

;
; Interfaces installation
;

;
; Audio
;

[AUD.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%KsNameFilter%,AUD_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%KsNameFilter%,AUD_Interface,
AddInterface={33d9a762-90c8-11d0-bd43-00a0c911ce86},%KsNameFilter%,AUD_Interface,

[AUD_Interface]
AddReg=AUD_Interface.AddReg

[AUD_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AUDFriendlyName%

;
; Services installation
;

[AUD.Services]
AddService = CXAVSAUD,2,AUD.ServiceInstall

[AUD.ServiceInstall]
DisplayName   = %CX23880.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\TV5083aud.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
KsNameFilter        = 	"{9B365890-165F-11D0-A195-0020AFD156E4}"

Proxy.CLSID         =   "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

CX23880.DeviceDesc  = 	"vp5083 Audio Capture"
AUDFriendlyName     =  	"vp5083 Audio Capture"
AudioPinID          =   "{27C304E1-80F6-11d5-AFD4-0001032B6C31}"
AudioPinName        =   "vp5083 Audio"

