;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;                                                                                       ;
; DC1120.inf -- Installation information for Syntek USB 2.0 DC-1120.                    ;
;                                                                                       ;
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Version]
signature="$CHICAGO$"
Class=Image
ClassGUID={6BDD1FC6-810F-11D0-BEC7-08002BE2092F}
Provider=%Company%
LayoutFile=Layout.inf, Layout1.inf, Layout2.inf
DriverVer=01/11/2005,1.0.0.1

[SourceDisksNames]
1=%StkDiskName%,,,

[SourceDisksFiles]
StkMini.sys = 1
StkCamd.sys = 1
StkPin.sys = 1
StkPipe.sys = 1
StkSam.sys = 1
StkScan.sys = 1
StkProp.ax = 1
StkTW.ds = 1
StkUSD.dll = 1
StkVFW.dll = 1
Stk112X.exe = 1

[ControlFlags]
; All PnP devices should be excluded from manual AddDevice Applet list
ExcludeFromSelect=*

[Manufacturer]
%UsbMfg%=SYNTEK

[DestinationDirs]
DefaultDestDir = 11
SYNTEK.USBDCAM.CopyDrivers98 = 10,system32\drivers
SYNTEK.USBDCAM.CopyDriversNT = 10,system32\drivers
SYNTEK.USBDCAM.CopyDrivers = 10,system32\drivers
SYNTEK.USBDCAM.CopyFilters = 11
SYNTEK.USBDCAM.CopyCodecs = 11
SYNTEK.STI.CopyFiles = 11
SYNTEK.STIAPP.CopyFiles = 10
SYNTEK.TWAIN.CopyFiles = 10,twain_32\DC112X

[SYNTEK]
;%StkMiniDescription%=SYNTEK.USBDCAM,USB\Vid_10f5&Pid_0004
%StkMiniDescription%=SYNTEK.USBDCAM,USB\Vid_10f5&Pid_0004&MI_00
;%StkMiniDescription%=SYNTEK.USBDCAM,USB\Vid_10f5&Pid_0004&MI_01
%StkMiniDescription%=SYNTEK.USBDCAM,USB\Vid_0932&Pid_0320&MI_00
%StkMiniDescription%=SYNTEK.USBDCAM,USB\Vid_0932&Pid_0300&MI_00

[SYNTEK.USBDCAM]
Include=ks.inf, kscaptur.inf, ksfilter.inf, dshowext.inf
Needs=KS.Registration, KSCAPTUR.Registration, DSHOWEXT.Registration
SubClass=StillImage
DeviceType=2
DeviceSubType=0x0
Capabilities=0x01
;PropertyPages="*.cpl ,EnumStiPropPages"
Events=SYNTEK.USBDCAM.Events
DeviceData=SYNTEK.USBDCAM.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"
AddReg=SYNTEK.USBDCAM.AddReg98,SYNTEK.USBDCAM.AddReg
UpdateInis=SYNTEK.USBDCAM.UpdateIni
CopyFiles=SYNTEK.USBDCAM.CopyDrivers98,SYNTEK.USBDCAM.CopyDrivers,SYNTEK.USBDCAM.CopyFilters,SYNTEK.USBDCAM.CopyCodecs,SYNTEK.STI.CopyFiles,SYNTEK.STIAPP.CopyFiles,SYNTEK.TWAIN.CopyFiles

[SYNTEK.USBDCAM.NT]
Include=ks.inf, kscaptur.inf, ksfilter.inf, dshowext.inf
Needs=KS.Registration, KSCAPTUR.Registration.NT, DSHOWEXT.Registration
SubClass=StillImage
DeviceType=2
DeviceSubType=0x0
Capabilities=0x01
;PropertyPages="*.cpl ,EnumStiPropPages"
Events=SYNTEK.USBDCAM.Events
DeviceData=SYNTEK.USBDCAM.DeviceData
ICMProfiles="sRGB Color Space Profile.icm"
AddReg=SYNTEK.USBDCAM.AddRegNT,SYNTEK.USBDCAM.AddReg
UpdateInis=SYNTEK.USBDCAM.UpdateIni
CopyFiles=SYNTEK.USBDCAM.CopyDriversNT,SYNTEK.USBDCAM.CopyDrivers,SYNTEK.USBDCAM.CopyFilters,SYNTEK.USBDCAM.CopyCodecs,SYNTEK.STI.CopyFiles,SYNTEK.STIAPP.CopyFiles,SYNTEK.TWAIN.CopyFiles

[SYNTEK.USBDCAM.AddReg98]
HKR,,NTMPDriver,,StkMini.sys

[SYNTEK.USBDCAM.AddRegNT]
HKR,,NTMPDriver,,StkMini.sys

[SYNTEK.USBDCAM.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,HardwareConfig,1,1
HKR,,PageOutWhenUnopened,3,01
; This is causing unexpected reset to our device.
; Put this line back when our device is able to handle the power down.
;HKR,,PowerDownWhenUnopened,3,01
;HKR,,DontSuspendIfStreamsAreRunning,3,00
HKR,"Settings","######",0x00010001,0xFF0000FF
HKR,"Settings","Board Vendor",0x00010001,0x00
HKR,"Settings","Board Type",0x00010001,0x00
HKR,"Settings","Power Saving",0x00010001,0x01
HKR,"Settings","Video Source",0x00010001,0x00
HKR,"Settings","Video Standard",0x00010001,0x01
HKR,"Settings","Audio Input Configuration",0x00010001,0x01
HKR,"Settings","Audio Output Configuration",0x00010001,0x03
HKR,"Settings","Video Input Configuration",0x00010001,0x01
HKR,"Settings","Video Output Configuration",0x00010001,0x01

; Default Settings
HKR,"Settings\Default\Decoder","Flip Horizontal",0x00010001,0x00
HKR,"Settings\Default\Decoder","Flip Vertical",0x00010001,0x00
HKR,"Settings\Default\Decoder","Audio Type",0x00010001,0x00
HKR,"Settings\Default\Decoder","Tuner Type",0x00010001,0x00
HKR,"Settings\Default\Decoder","VBI",0x00010001,0x00
HKR,"Settings\Default\Decoder","VBI Format",0x00010001,0x55
HKR,"Settings\Default\Decoder","Brightness",0x00010001,0x80
HKR,"Settings\Default\Decoder","Contrast",0x00010001,0x40
HKR,"Settings\Default\Decoder","Hue",0x00010001,0xB4
HKR,"Settings\Default\Decoder","Saturation",0x00010001,0x100
HKR,"Settings\Default\Decoder","Sharpness",0x00010001,0x03
HKR,"Settings\Default\Decoder","Gamma",0x00010001,0x1A
HKR,"Settings\Default\Decoder","White Balance",0x00010001,0x80
HKR,"Settings\Default\Decoder","Back Light",0x00010001,0x80
HKR,"Settings\Default\Decoder","Color Enable",0x00010001,0x00
HKR,"Settings\Default\Decoder","AWB",0x00010001,0x00
HKR,"Settings\Default\Decoder","Tuner Auto Scan Enable",0x00010001,0x00
HKR,"Settings\Default\Decoder","Tuner TV Standard",0x00010001,0x01

HKR,"Settings\Default\Sensor","Flip Horizontal",0x00010001,0x00
HKR,"Settings\Default\Sensor","Flip Vertical",0x00010001,0x00
HKR,"Settings\Default\Sensor","AE",0x00010001,0x01
HKR,"Settings\Default\Sensor","AE Mode",0x00010001,0x00
HKR,"Settings\Default\Sensor","AE Range",0x00010001,0xFF
HKR,"Settings\Default\Sensor","AE Level",0x00010001,0x80
HKR,"Settings\Default\Sensor","Low Light",0x00010001,0x00
HKR,"Settings\Default\Sensor","Low Light Limit",0x00010001,0x4000
HKR,"Settings\Default\Sensor","High Light",0x00010001,0x00
HKR,"Settings\Default\Sensor","Light Flicker",0x00010001,0x01
HKR,"Settings\Default\Sensor","Quality",0x00010001,0x04
HKR,"Settings\Default\Sensor","AWB Mode",0x00010001,0x00
HKR,"Settings\Default\Sensor","Incandescent RB Gain",0x00010001,0x00DF019F
HKR,"Settings\Default\Sensor","Fluorescent RB Gain",0x00010001,0x01940133
HKR,"Settings\Default\Sensor","Daylight RB Gain",0x00010001,0x015A0128
HKR,"Settings\Default\Sensor","Monitor",0x00010001,0x00
HKR,"Settings\Default\Sensor","Frame Rate Control",0x00010001,0x00
HKR,"Settings\Default\Sensor","Auto Flip Vertical",0x00010001,0x00
HKR,"Settings\Default\Sensor","Sensor Output Format",0x00010001,0x00
HKR,"Settings\Default\Sensor\CRT","Brightness",0x00010001,0x80
HKR,"Settings\Default\Sensor\CRT","Contrast",0x00010001,0x40
HKR,"Settings\Default\Sensor\CRT","Hue",0x00010001,0xB4
HKR,"Settings\Default\Sensor\CRT","Saturation",0x00010001,0x100
HKR,"Settings\Default\Sensor\CRT","Sharpness",0x00010001,0x03
HKR,"Settings\Default\Sensor\CRT","Gamma",0x00010001,0x1A
HKR,"Settings\Default\Sensor\CRT","White Balance",0x00010001,0x05
HKR,"Settings\Default\Sensor\CRT","Back Light",0x00010001,0x80
HKR,"Settings\Default\Sensor\CRT","Color Enable",0x00010001,0x00
HKR,"Settings\Default\Sensor\CRT","AWB",0x00010001,0x01
HKR,"Settings\Default\Sensor\LCD","Brightness",0x00010001,0x80
HKR,"Settings\Default\Sensor\LCD","Contrast",0x00010001,0x40
HKR,"Settings\Default\Sensor\LCD","Hue",0x00010001,0xB4
HKR,"Settings\Default\Sensor\LCD","Saturation",0x00010001,0x100
HKR,"Settings\Default\Sensor\LCD","Sharpness",0x00010001,0x03
HKR,"Settings\Default\Sensor\LCD","Gamma",0x00010001,0x1A
HKR,"Settings\Default\Sensor\LCD","White Balance",0x00010001,0x05
HKR,"Settings\Default\Sensor\LCD","Back Light",0x00010001,0x80
HKR,"Settings\Default\Sensor\LCD","Color Enable",0x00010001,0x00
HKR,"Settings\Default\Sensor\LCD","AWB",0x00010001,0x01

; Current Settings
HKR,"Settings\Current\Decoder","Flip Horizontal",0x00010001,0x00
HKR,"Settings\Current\Decoder","Flip Vertical",0x00010001,0x00
HKR,"Settings\Current\Decoder","Audio Type",0x00010001,0x00
HKR,"Settings\Current\Decoder","Tuner Type",0x00010001,0x00
HKR,"Settings\Current\Decoder","VBI",0x00010001,0x00
HKR,"Settings\Current\Decoder","VBI Format",0x00010001,0x55
HKR,"Settings\Current\Decoder","Brightness",0x00010001,0x80
HKR,"Settings\Current\Decoder","Contrast",0x00010001,0x40
HKR,"Settings\Current\Decoder","Hue",0x00010001,0xB4
HKR,"Settings\Current\Decoder","Saturation",0x00010001,0x100
HKR,"Settings\Current\Decoder","Sharpness",0x00010001,0x03
HKR,"Settings\Current\Decoder","Gamma",0x00010001,0x1A
HKR,"Settings\Current\Decoder","White Balance",0x00010001,0x80
HKR,"Settings\Current\Decoder","Back Light",0x00010001,0x80
HKR,"Settings\Current\Decoder","Color Enable",0x00010001,0x00
HKR,"Settings\Current\Decoder","AWB",0x00010001,0x00
HKR,"Settings\Current\Decoder","Tuner Auto Scan Enable",0x00010001,0x00
HKR,"Settings\Current\Decoder","Tuner TV Standard",0x00010001,0x01

HKR,"Settings\Current\Sensor","Flip Horizontal",0x00010001,0x00
HKR,"Settings\Current\Sensor","Flip Vertical",0x00010001,0x00
HKR,"Settings\Current\Sensor","AE",0x00010001,0x01
HKR,"Settings\Current\Sensor","AE Mode",0x00010001,0x00
HKR,"Settings\Current\Sensor","AE Range",0x00010001,0xFF
HKR,"Settings\Current\Sensor","AE Level",0x00010001,0x80
HKR,"Settings\Current\Sensor","Low Light",0x00010001,0x00
HKR,"Settings\Current\Sensor","Low Light Limit",0x00010001,0x4000
HKR,"Settings\Current\Sensor","High Light",0x00010001,0x00
HKR,"Settings\Current\Sensor","Light Flicker",0x00010001,0x01
HKR,"Settings\Current\Sensor","Quality",0x00010001,0x04
HKR,"Settings\Current\Sensor","AWB Mode",0x00010001,0x00
HKR,"Settings\Current\Sensor","Incandescent RB Gain",0x00010001,0x00DF019F
HKR,"Settings\Current\Sensor","Fluorescent RB Gain",0x00010001,0x01940133
HKR,"Settings\Current\Sensor","Daylight RB Gain",0x00010001,0x015A0128
HKR,"Settings\Current\Sensor","Monitor",0x00010001,0x00
HKR,"Settings\Current\Sensor","Frame Rate Control",0x00010001,0x00
HKR,"Settings\Current\Sensor","Auto Flip Vertical",0x00010001,0x00
HKR,"Settings\Current\Sensor","Sensor Output Format",0x00010001,0x00
HKR,"Settings\Current\Sensor\CRT","Brightness",0x00010001,0x80
HKR,"Settings\Current\Sensor\CRT","Contrast",0x00010001,0x40
HKR,"Settings\Current\Sensor\CRT","Hue",0x00010001,0xB4
HKR,"Settings\Current\Sensor\CRT","Saturation",0x00010001,0x100
HKR,"Settings\Current\Sensor\CRT","Sharpness",0x00010001,0x03
HKR,"Settings\Current\Sensor\CRT","Gamma",0x00010001,0x1A
HKR,"Settings\Current\Sensor\CRT","White Balance",0x00010001,0x05
HKR,"Settings\Current\Sensor\CRT","Back Light",0x00010001,0x80
HKR,"Settings\Current\Sensor\CRT","Color Enable",0x00010001,0x00
HKR,"Settings\Current\Sensor\CRT","AWB",0x00010001,0x01
HKR,"Settings\Current\Sensor\LCD","Brightness",0x00010001,0x80
HKR,"Settings\Current\Sensor\LCD","Contrast",0x00010001,0x40
HKR,"Settings\Current\Sensor\LCD","Hue",0x00010001,0xB4
HKR,"Settings\Current\Sensor\LCD","Saturation",0x00010001,0x100
HKR,"Settings\Current\Sensor\LCD","Sharpness",0x00010001,0x03
HKR,"Settings\Current\Sensor\LCD","Gamma",0x00010001,0x1A
HKR,"Settings\Current\Sensor\LCD","White Balance",0x00010001,0x05
HKR,"Settings\Current\Sensor\LCD","Back Light",0x00010001,0x80
HKR,"Settings\Current\Sensor\LCD","Color Enable",0x00010001,0x00
HKR,"Settings\Current\Sensor\LCD","AWB",0x00010001,0x01

; Still Image
HKR,,USDClass,,"{89FE3F30-23E1-450A-84F2-9CD69ABAB63E}"
HKCR,CLSID\{89FE3F30-23E1-450A-84F2-9CD69ABAB63E},,,"Syntek USD"
HKCR,CLSID\{89FE3F30-23E1-450A-84F2-9CD69ABAB63E}\InProcServer32,,,%11%\StkUSD.dll
HKCR,CLSID\{89FE3F30-23E1-450A-84F2-9CD69ABAB63E}\InProcServer32,ThreadingModel,,"Both"

; Register the name of application
HKLM,"Software\Microsoft\Windows\CurrentVersion\StillImage\Registered Applications",%StillAPP%,,"%10%\Stk112X.exe /StiDevice:%1 /StiEvent:%2"
HKLM,"Software\Microsoft\Windows NT\CurrentVersion\DC112X","DeviceName",,"%StkMiniDescription%"

; Register DC-112X Property Page

; Plug-In Custom Control Interface
HKCR,CLSID\{59DF6360-6F14-4472-82B6-6EAB971EEFAD},,,%PlugIn_CustomControlInterface%
HKCR,CLSID\{59DF6360-6F14-4472-82B6-6EAB971EEFAD}\InprocServer32,,,StkProp.ax
HKCR,CLSID\{59DF6360-6F14-4472-82B6-6EAB971EEFAD}\InprocServer32,ThreadingModel,,Both
; This IID is aggregated for the filter given the CLSID of the property set
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{59DF6360-6F14-4472-82B6-6EAB971EEFAD},,,%PlugIn_CustomControlInterface%
HKLM,System\CurrentControlSet\Control\MediaInterfaces\{59DF6360-6F14-4472-82B6-6EAB971EEFAD},IID,1,60,63,DF,59,14,6F,72,44,82,B6,6E,AB,97,1E,EF,AD

; Plug-In Custom Control Property Page
HKCR,CLSID\{59DF6361-6F14-4472-82B6-6EAB971EEFAD},,,%PlugIn_CustomControlPropertyPage%
HKCR,CLSID\{59DF6361-6F14-4472-82B6-6EAB971EEFAD}\InprocServer32,,,StkProp.ax
HKCR,CLSID\{59DF6361-6F14-4472-82B6-6EAB971EEFAD}\InprocServer32,ThreadingModel,,Both
; Associate the property set with the above property page
HKLM,System\CurrentControlSet\Control\MediaSets\{59DF6360-6F14-4472-82B6-6EAB971EEFAD}\PropertyPages\{59DF6361-6F14-4472-82B6-6EAB971EEFAD},,,%PlugIn_CustomControlPropertyPage%

[SYNTEK.USBDCAM.HW]
AddReg=SYNTEK_USBDCAM_AddFilter

[SYNTEK_USBDCAM_AddFilter]
HKR,,"UpperFilters",0x00000000,"StkScan.sys"

[SYNTEK.USBDCAM.NT.HW]
AddReg=SYNTEK_USBDCAM_NT_AddFilter

[SYNTEK_USBDCAM_NT_AddFilter]
HKR,,"UpperFilters",0x00010000,"StkScan"

[SYNTEK.USBDCAM.DeviceData]
TwainDS=%TwainDsName%
SpecialInfo="UsbPC 2.0"

[SYNTEK.USBDCAM.Events]
NewPicture=%NewPicture%,{89FE3F31-23E1-450A-84F2-9CD69ABAB63E},%StillAPP%
ButtonPressed=%ButtonPressed%,{89FE3F32-23E1-450A-84F2-9CD69ABAB63E},%StillAPP%

[SYNTEK.USBDCAM.UpdateIni]
system.ini,drivers32,,"VIDC.I420=MSh263.drv"

[SYNTEK.USBDCAM.CopyDrivers98]
StkMini.sys
StkCamd.sys

[SYNTEK.USBDCAM.CopyDriversNT]
StkMini.sys
StkCamd.sys

[SYNTEK.USBDCAM.CopyDrivers]
StkPin.sys
StkPipe.sys
StkSam.sys
StkScan.sys

[SYNTEK.USBDCAM.CopyCodecs]
StkProp.ax
StkVFW.dll

[SYNTEK.USBDCAM.CopyFilters]

[SYNTEK.STI.CopyFiles]
StkUSD.dll

[SYNTEK.STIAPP.CopyFiles]
Stk112X.exe

[SYNTEK.TWAIN.CopyFiles]
StkTW.ds

[SYNTEK.USBDCAM.Interfaces]
AddInterface={65E8773D-8F56-11D0-A3B9-00A0C9223196},GLOBAL,Capture.Interface
AddInterface={A799A800-A46D-11D0-A18c-00A02401DCD4},GLOBAL,TVTuner.Interface
AddInterface={A799A801-A46D-11D0-A18C-00A02401DCD4},GLOBAL,CrossBar.Interface
AddInterface={A799A802-A46D-11D0-A18C-00A02401DCD4},GLOBAL,TVAudio.Interface

[SYNTEK.USBDCAM.NT.Interfaces]
AddInterface={65E8773D-8F56-11D0-A3B9-00A0C9223196},GLOBAL,Capture.Interface
AddInterface={A799A800-A46D-11D0-A18c-00A02401DCD4},GLOBAL,TVTuner.Interface
AddInterface={A799A801-A46D-11D0-A18C-00A02401DCD4},GLOBAL,CrossBar.Interface
AddInterface={A799A802-A46D-11D0-A18C-00A02401DCD4},GLOBAL,TVAudio.Interface

[Capture.Interface]
AddReg=Capture.AddReg

[TVTuner.Interface]
AddReg=TVTuner.AddReg

[CrossBar.Interface]
AddReg=CrossBar.AddReg

[TVAudio.Interface]
AddReg=TVAudio.AddReg

[Capture.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%StkMiniDescription%
HKR,,ExtensionDLL,,StkVFW.dll
HKLM,Software\CLASSES\CLSID\{DA4E3DA0-D07D-11D0-BD50-00A0C911CE86}\Instance\{07DAD660-22F1-11D1-A9F4-00C04FBBDE8F}
HKLM,Software\CLASSES\CLSID\{DA4E3DA0-D07D-11D0-BD50-00A0C911CE86}\Instance\{07DAD660-22F1-11D1-A9F4-00C04FBBDE8F},,,"WDM Streaming VBI Codecs"
HKLM,Software\CLASSES\CLSID\{DA4E3DA0-D07D-11D0-BD50-00A0C911CE86}\Instance\{07DAD660-22F1-11D1-A9F4-00C04FBBDE8F},FriendlyName,,"WDM Streaming VBI Codecs"
HKLM,Software\CLASSES\CLSID\{DA4E3DA0-D07D-11D0-BD50-00A0C911CE86}\Instance\{07DAD660-22F1-11D1-A9F4-00C04FBBDE8F},CLSID,,{07DAD660-22F1-11D1-A9F4-00C04FBBDE8F}
HKR,PinFactory\1\Interfaces\{5BB95400-52BB-11D2-BA41-00A0C90D2B05},,,

[TVTuner.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11CF-8A03-00AA006ECB65}
HKR,,FriendlyName,,%TvTunerFilterName%

[CrossBar.AddReg]
HKR,,CLSID,,{71F96460-78F3-11D0-A18C-00A0C9118956}
HKR,,FriendlyName,,%CrossBarFilterName%

[TVAudio.AddReg]
HKR,,CLSID,,{71F96462-78F3-11D0-A18C-00A0C9118956}
HKR,,FriendlyName,,%TvAudioFilterName%

[SYNTEK.USBDCAM.NT.Services]
AddService=StkMini,0x00000002,SYNTEK.USBDCAM.Install.Mini
AddService=StkScan,0x00000000,SYNTEK.USBDCAM.Install.Scan

[SYNTEK.USBDCAM.Install.Mini]
DisplayName   = %StkMiniDescription%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\System32\Drivers\StkMini.sys

[SYNTEK.USBDCAM.Install.Scan]
DisplayName   = %StkScanDescription%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\System32\Drivers\StkScan.sys

[Strings]

;----------------
; Non-Localizable
;----------------
SERVICE_KERNEL_DRIVER=1
; PnP should use demand start
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1

;----------------
; Localizable
;----------------
Company="Turtle Beach Inc."
UsbMfg="Turtle Beach Inc."
StkDiskName="VideoAdvantage USB Driver Disk"
StkMiniDescription="VideoAdvantage USB"
StkScanDescription="VideoAdvantage Still Image"
PlugIn_CustomControlInterface="Syntek Custom Control Interface"
PlugIn_CustomControlPropertyPage="Syntek Custom Control Property Page"
NewPicture="New Picture Captured"
ButtonPressed="Button Pressed"
TwainDsName="VideoAdvantage USB TWAIN Image Capture"
StillAPP="VideoAdvantage USB Image Capture"
TvTunerFilterName  = "VideoAdvantage TvTuner"
CrossBarFilterName = "VideoAdvantage CrossBar"
TvAudioFilterName  = "VideoAdvantage TvAudio"
